For 1990-2009 cars

Callout | Component Name
--- | ---

#### Preliminary Procedure

1. Remove the steering wheel. Refer to Steering Wheel Replacement .
2. Remove the steering column trim covers. Refer to Steering Column Trim Covers Replacement .

1 | Inflatable Restraint Steering Wheel Module Coil Screw Notice: Refer to Fastener Notice in the Preface section. Tighten 1.5 N·m (13 lb in)
2 | Inflatable Restraint Steering Wheel Module Coil Assembly