For 1990-2009 cars

This master DTC list includes all applicable DTCs in alphanumeric order with descriptors.

DTC | DTC Descriptor | Module That Sets the DTC | Diagnostic Procedure
--- | --- | --- | ---
Important: Do not clear any DTCs unless instructed to do so by a diagnostic procedure. Important: If any DTCs are Powertrain related DTCs, select Capture Info in order to store the DTC information with the scan tool. Diagnose any current DTCs in the following order:

1. DTCs that begin with a U.
2. Any of the following: B1000, B1001, B1004, B1009, B1019, C0550, C0551, C0561, C0569, P0601, P0602, P0603, P0604, P0606, P0607, P060D, P062B, P062F, P167A, P167D, P2105, P2107, or P2610.
3. Any of the following: B1325, B1370, B1441, C0899, C0900, P0560, P0562, or P0563.
4. Component level DTCs.
5. System level DTCs.
6. Any remaining DTCs.

B0012 | Driver Frontal Deployment Loop Stage 1 | SDM | DTC B0012 or B0013
B0013 | Driver Frontal Deployment Loop Stage 2 | SDM | DTC B0012 or B0013
B0015 | Left Front Seat Belt Pretensioner Deployment Loop | SDM | DTC B0014-B0045
B0019 | Passenger Frontal Deployment Loop Stage 1 | SDM | DTC B0014-B0045
B0020 | Passenger Frontal Deployment Loop Stage 2 | SDM | DTC B0014-B0045
B0022 | Right Front Seat Belt Pretensioner Deployment Loop | SDM | DTC B0014-B0045
B0052 | Deployment Commanded | SDM | DTC B0052 or B0053
B0053 | Deployment Commanded with Loop DTCs Present | SDM | DTC B0052 or B0053
B0081 | Passenger Presence System | SDM | DTC B0081
B0083 | Front End Sensor 1 | SDM | DTC B0083 or B0084
B0084 | Front End Sensor 2 | SDM | DTC B0083 or B0084
B0283 | Electric Rear Defrost Circuit | BCM | DTC B0283
B1000 | Electronic Control Unit (ECU) Performance | BCM, DRR, IPC, Radio, RCDLR, SDM, TDM | DTC B1000
B1001 | Option Configuration Error | BCM | DTC B1001
SDM | DTC B1001
B1004 | Keep Alive Memory (KAM) Reset | BCM | DTC B1004
B1009 | EEPROM Checksum Mismatch | BCM | DTC B1009
B1019 | System Configuration Error | SDM | DTC B1019
B1025 | LF Audio Output Circuit | Radio | DTC B1025, B1035, B1045, or B1055
B1035 | RF Audio Output Circuit | Radio | DTC B1025, B1035, B1045, or B1055
B1045 | LR Audio Output Circuit | Radio | DTC B1025, B1035, B1045, or B1055
B1055 | RR Audio Output Circuit | Radio | DTC B1025, B1035, B1045, or B1055
B1287 | External Amp Control | Radio | DTC B1287
B1325 | Device Power 1 Circuit | BCM, IPC, Radio, SDM | DTC B1325
B1370 | Device Ignition 1 Circuit | BCM | DTC B1370
SDM | DTC B1370
B1380 | Device Ignition ACCESSORY Circuit | BCM | DTC B1380
B1441 | Device Ignition OFF, RUN, and CRANK Circuit | BCM | DTC B1441
B1480 | Battery Rundown Protection Circuit | BCM | DTC B1480
B2455 | Cellular Phone Microphone Circuit | VCIM | DTC B2455
B2470 | Cellular Phone Antenna Circuit | VCIM | DTC B2470
B2476 | Cellular Phone Select Service Switch | VCIM | DTC B2476
B2482 | Cellular Phone Select Service Switch Performance | VCIM | DTC B2482
B2483 | Global Positioning System (GPS) Sensor Circuit Low | VCIM | DTC B2483 or B2484
B2484 | Global Positioning System (GPS) Sensor Circuit Open | VCIM | DTC B2483 or B2484
B2530 | Front Fog Lamps Control Circuit | BCM | DTC B2530
B2555 | Passenger Compartment Lamp Control Circuit | BCM | DTC B2555
B2580 | Headlamp High Beam Control Circuit | BCM | DTC B2580
B2625 | Display Dimming Pulse Width Modulation (PWM) Output Circuit | BCM | DTC B2625
B2645 | Ambient Light Sensor Circuit | BCM | DTC B2645
B2705 | Gearshift Unlock Circuit | BCM | DTC B2705
B2750 | Horn Relay Coil Circuit | BCM | DTC B2750
B2961 | Key In Ignition Circuit | BCM | DTC B2961
B3031 | Security System Controller In Learn Mode | VTD | DTC B3031
B3055 | No Transponder Modulation or No Transponder | VTD | DTC B3055
B3060 | Unprogrammed Transponder Identification Code Received | VTD | DTC B3060
B3105 | Keyless Entry System Key Fobs Not Programmed | RCDLR | DTC B3105
B3109 | Keyless Entry Transmitter 1 Low Battery | RCDLR | DTC B3109, B3110, B3111, or B3112
B3110 | Keyless Entry Transmitter 2 Low Battery | RCDLR | DTC B3109, B3110, B3111, or B3112
B3111 | Keyless Entry Transmitter 3 Low Battery | RCDLR | DTC B3109, B3110, B3111, or B3112
B3112 | Keyless Entry Transmitter 4 Low Battery | RCDLR | DTC B3109, B3110, B3111, or B3112
B3265 | Trunk Relay Output | BCM | DTC B3265
B3715 | Front Wiper Relay Drive Circuit | BCM | DTC B3715
B3794 | Cruise Control Function Request Circuit | BCM | DTC B3794
B3903 | Stop Lamp Relay Circuit | BCM | DTC B3903
B3935 | Transponder Authentication Error | VTD | DTC B3935
B3948 | Left Front Turn Signal Circuit | BCM | DTC B3948 or B3949
B3949 | Right Front Turn Signal Circuit | BCM | DTC B3948 or B3949
B3950 | Left Rear Turn Signal Circuit | BCM | DTC B3950 or B3951
B3951 | Right Rear Turn Signal Circuit | BCM | DTC B3950 or B3951
B3976 | Unconfigured Transponder | VTD | DTC B3976
C0035 | Left Front Wheel Speed Sensor Circuit | EBCM | DTC C0035-C0050
C0040 | Right Front Wheel Speed Sensor Circuit | EBCM | DTC C0035-C0050
C0045 | Left Rear Wheel Speed Sensor Circuit | EBCM | DTC C0035-C0050
C0050 | Right Rear Wheel Speed Sensor Circuit | EBCM | DTC C0035-C0050
C0110 | Pump Motor Circuit | EBCM | DTC C0110
C0131 | Antilock Brake System (ABS) Pressure Circuit | EBCM | DTC C0131
C0161 | Antilock Brake System (ABS)/Traction Control System (TCS) Brake Switch Circuit Signal Malfunction | EBCM | DTC C0161
C0186 | Lateral Accelerometer Circuit | EBCM | DTC C0186
C0196 | Yaw Rate Circuit | EBCM | DTC C0196
C0201 | Antilock Brake System (ABS) Enable Relay Contact Circuit | EBCM | DTC C0201
C0252 | Vehicle Stability Enhancement System (VSES) Sensors Uncorrelated | EBCM | DTC C0252
C0267 | Low Brake Fluid Indicated | EBCM | DTC C0267
C0277 | Brake Pedal Position Sensor Circuit | BCM | DTC C0277
C0278 | Brake Pedal Position Sensor Not Calibrated | BCM | DTC C0278
C0292 | VSES Combination Sensor Circuits | EBCM | DTC C0292
C0460 | Steering Position Sensor | EBCM | DTC C0460
C0550 | Electronic Control Unit (ECU) Performance | EBCM | DTC C0550 or DTC C0550
C0551 | Option Configuration Error | EBCM | DTC C0551
C0561 | System Disabled Information Stored | EBCM | DTC C0561
C0569 | System Configuration Error | EBCM | DTC C0569
C0870 | Device Voltage Reference Output 1 | BCM | DTC C0870
C0899 | Device Voltage Low | EBCM | DTC C0899
C0900 | Device Voltage High | EBCM | DTC C0900
P0010 | Intake Camshaft Position (CMP) Actuator Solenoid Control Circuit | ECM | DTC P0010 or P0011 for the 2.0L engine or DTC P0010, P0011, P0013, or P0014 for the 2.4L engine
P0011 | Intake Camshaft Position (CMP) System Performance | ECM | DTC P0010 or P0011 for the 2.0L engine or DTC P0010, P0011, P0013, or P0014 for the 2.4L engine
P0013 | Exhaust Camshaft Position (CMP) Actuator Solenoid Control Circuit | ECM | DTC P0013 or P0014 for the 2.0L engine or DTC P0010, P0011, P0013, or P0014 for the 2.4L engine
P0014 | Exhaust Camshaft Position (CMP) System Performance | ECM | DTC P0013 or P0014 for the 2.0L engine or DTC P0010, P0011, P0013, or P0014 for the 2.4L engine
P0016 | Crankshaft Position (CKP) - Intake Camshaft Position (CMP) Correlation | ECM | DTC P0016 or P0017 for the 2.0L engine or DTC P0016 for the 2.4L engine
P0017 | Crankshaft Position (CKP) - Exhaust Camshaft Position (CMP) Correlation | ECM | DTC P0016 or P0017 for the 2.0L engine or DTC P0017 for the 2.4L engine
P0030 | HO2S Heater Control Circuit Sensor 1 | ECM | DTC P0030, P0031, P0032, P0053, or P0135 for the 2.0L engine or DTC P0030, P0036, P0053, P0054, P0135, or P0141 for the 2.4L engine
P0031 | HO2S Heater Control Circuit Low Voltage Sensor 1 | ECM | DTC P0030, P0031, P0032, P0053, or P0135 for the 2.0L engine
P0032 | HO2S Heater Control Circuit High Voltage Sensor 1 | ECM | DTC P0030, P0031, P0032, P0053, or P0135 for the 2.0L engine
P0033 | Turbocharger Bypass Valve Solenoid Control Circuit | ECM | DTC P0033, P0034, or P0035 for the 2.0L engine
P0034 | Turbocharger Bypass Valve Solenoid Control Circuit Low Voltage | ECM | DTC P0033, P0034, or P0035 for the 2.0L engine
P0035 | Turbocharger Bypass Valve Solenoid Control Circuit High Voltage | ECM | DTC P0033, P0034, or P0035 for the 2.0L engine
P0036 | HO2S Heater Control Circuit Sensor 2 | ECM | DTC P0036, P0037, P0038, or P0141 for the 2.0L engine or DTC P0030, P0036, P0053, P0054, P0135, or P0141 for the 2.4L engine
P0037 | HO2S Heater Control Circuit Low Voltage Sensor 2 | ECM | DTC P0036, P0037, P0038, or P0141 for the 2.0L engine
P0038 | HO2S Heater Control Circuit High Voltage Sensor 2 | ECM | DTC P0036, P0037, P0038, or P0141 for the 2.0L engine
P0053 | HO2S Heater Resistance Sensor 1 | ECM | DTC P0030, P0031, P0032, P0053, or P0135 for the 2.0L engine or DTC P0030, P0036, P0053, P0054, P0135, or P0141 for the 2.4L engine
P0054 | HO2S Heater Resistance Sensor 2 | ECM | DTC P0030, P0036, P0053, P0054, P0135, or P0141 for the 2.4L engine
P0068 | Throttle Body Airflow Performance | ECM | DTC P0068 or P0121 for the 2.4L engine
P0087 | Fuel Rail Pressure (FRP) Too Low | ECM | DTC P0087, P0088, or P0089 for the 2.0L engine
P0088 | Fuel Rail Pressure (FRP) Too High | ECM | DTC P0087, P0088, or P0089 for the 2.0L engine
P0089 | Fuel Pressure Regulator Performance | ECM | DTC P0087, P0088, or P0089 for the 2.0L engine
P0090 | Fuel Pressure Regulator Control Circuit | ECM | DTC P0090, P0091, or P0092 for the 2.0L engine
P0091 | Fuel Pressure Regulator Solenoid 1 Control Circuit Low Voltage | ECM | DTC P0090, P0091, or P0092 for the 2.0L engine
P0092 | Fuel Pressure Regulator Solenoid 1 Control Circuit High Voltage | ECM | DTC P0090, P0091, or P0092 for the 2.0L engine
P0096 | Intake Air Temperature (IAT) Sensor 2 Performance | ECM | DTC P0096, P0097, P0098, or P0099 for the 2.0L engine
P0097 | Intake Air Temperature (IAT) Sensor 2 Circuit Low Voltage | ECM | DTC P0096, P0097, P0098, or P0099 for the 2.0L engine
P0098 | Intake Air Temperature (IAT) Sensor 2 Circuit High Voltage | ECM | DTC P0096, P0097, P0098, or P0099 for the 2.0L engine
P0099 | Intake Air Temperature (IAT) Sensor 2 Circuit Intermittent | ECM | DTC P0096, P0097, P0098, or P0099 for the 2.0L engine
P0100 | Mass Air Flow (MAF) Sensor Circuit | ECM | DTC P0100, P0101, P0102, or P0103 for the 2.0L engine
P0101 | Mass Air Flow (MAF) Sensor Performance | ECM | DTC P0100, P0101, P0102, or P0103 for the 2.0L engine or DTC P0101 or P1101 for the 2.4L engine
P0102 | Mass Air Flow (MAF) Sensor Circuit Low Frequency | ECM | DTC P0100, P0101, P0102, or P0103 for the 2.0L engine or DTC P0102 or P0103 for the 2.4L engine
P0103 | Mass Air Flow (MAF) Sensor Circuit High Frequency | ECM | DTC P0100, P0101, P0102, or P0103 for the 2.0L engine or DTC P0102 or P0103 for the 2.4L engine
P0106 | Manifold Absolute Pressure (MAP) Sensor Performance | ECM | DTC P0106, P0107, or P0108 for the 2.0L engine or DTC P0106 for the 2.4L engine
P0107 | Manifold Absolute Pressure (MAP) Sensor Circuit Low Voltage | ECM | DTC P0106, P0107, or P0108 for the 2.0L engine or DTC P0107 or P0108 for the 2.4L engine
P0108 | Manifold Absolute Pressure (MAP) Sensor Circuit High Voltage | ECM | DTC P0106, P0107, or P0108 for the 2.0L engine or DTC P0107 or P0108 for the 2.4L engine
P0112 | Intake Air Temperature (IAT) Sensor Circuit Low Voltage | ECM | DTC P0112, P0113, or P0114 for the 2.0L engine or DTC P0112 or P0113 for the 2.4L engine
P0113 | Intake Air Temperature (IAT) Sensor Circuit High Voltage | ECM | DTC P0112, P0113, or P0114 for the 2.0L engine or DTC P0112 or P0113 for the 2.4L engine
P0114 | Intake Air Temperature (IAT) Sensor Circuit Intermittent | ECM | DTC P0112, P0113, or P0114 for the 2.0L engine
P0115 | Engine Coolant Temperature (ECT) Sensor Circuit | TCM | DTC P0115
P0116 | Engine Coolant Temperature (ECT) Sensor Performance | ECM | DTC P0116 for the 2.0L engine or DTC P0116 for the 2.4L engine
P0117 | Engine Coolant Temperature (ECT) Sensor Circuit Low Voltage | ECM | DTC P0117, P0118, or P0119 for the 2.0L engine or DTC P0117 or P0118 for the 2.4L engine
P0118 | Engine Coolant Temperature (ECT) Sensor Circuit High Voltage | ECM | DTC P0117, P0118, or P0119 for the 2.0L engine or DTC P0117 or P0118 for the 2.4L engine
P0119 | Engine Coolant Temperature (ECT) Sensor Circuit Intermittent | ECM | DTC P0117, P0118, or P0119 for the 2.0L engine
P0120 | Throttle Position (TP) Sensor Circuit | TCM | DTC P0120
Throttle Position (TP) Sensor 1 Circuit | ECM | DTC P0120, P0122, P0123, P0220, P0222, P0223, or P2135 for the 2.4L engine
P0121 | Throttle Position (TP) Sensor Performance | ECM | DTC P0121, P0122, or P0123 for the 2.0L engine or DTC P0068 or P0121 for the 2.4L engine
P0122 | Throttle Position (TP) Sensor 1 Circuit Low Voltage | ECM | DTC P0121, P0122, or P0123 for the 2.0L engine or DTC P0120, P0122, P0123, P0220, P0222, P0223, or P2135 for the 2.4L engine
P0123 | Throttle Position (TP) Sensor 1 Circuit High Voltage | ECM | DTC P0121, P0122, or P0123 for the 2.0L engine or DTC P0120, P0122, P0123, P0220, P0222, P0223, or P2135 for the 2.4L engine
P0125 | Engine Coolant Temperature (ECT) Insufficient For Closed Loop Fuel Control | ECM | DTC P0125 or P0128 for the 2.0L engine
P0128 | Engine Coolant Temperature (ECT) Below Thermostat Regulating Temperature | ECM | DTC P0125 or P0128 for the 2.0L engine or DTC P0128 for the 2.4L engine
P0130 | HO2S Circuit Closed Loop (CL) Performance Sensor 1 | ECM | DTC P0130, P0131, P0132, P0133, P2195, P2196, P2231, or P2297 for the 2.0L engine
P0131 | HO2S Circuit Low Voltage Sensor 1 | ECM | DTC P0130, P0131, P0132, P0133, P2195, P2196, P2231, or P2297 for the 2.0L engine or DTC P0131, P0132, P0137, or P0138 for the 2.4L engine
P0132 | HO2S Circuit High Voltage Sensor 1 | ECM | DTC P0130, P0131, P0132, P0133, P2195, P2196, P2231, or P2297 for the 2.0L engine or DTC P0131, P0132, P0137, or P0138 for the 2.4L engine
P0133 | HO2S Slow Response Sensor 1 | ECM | DTC P0130, P0131, P0132, P0133, P2195, P2196, P2231, or P2297 for the 2.0L engine or DTC P0133, P0134, P0140, P1133, P2A00, or P2A01 for the 2.4L engine
P0134 | HO2S Circuit Insufficient Activity Sensor 1 | ECM | DTC P0133, P0134, P0140, P1133, P2A00, or P2A01 for the 2.4L engine
P0135 | HO2S Heater Performance Sensor 1 | ECM | DTC P0030, P0031, P0032, P0053, or P0135 for the 2.0L engine or DTC P0030, P0036, P0053, P0054, P0135, or P0141 for the 2.4L engine
P0137 | HO2S Circuit Low Voltage Sensor 2 | ECM | DTC P0137, P0138, P0139, P0140, P2232, P2270, or P2271 for the 2.0L engine or DTC P0131, P0132, P0137, or P0138 for the 2.4L engine
P0138 | HO2S Circuit High Voltage Sensor 2 | ECM | DTC P0137, P0138, P0139, P0140, P2232, P2270, or P2271 for the 2.0L engine or DTC P0131, P0132, P0137, or P0138 for the 2.4L engine
P0139 | HO2S Slow Response Sensor 2 | ECM | DTC P0137, P0138, P0139, P0140, P2232, P2270, or P2271 for the 2.0L engine
P0140 | HO2S Circuit Insufficient Activity Sensor 2 | ECM | DTC P0137, P0138, P0139, P0140, P2232, P2270, or P2271 for the 2.0L engine or DTC P0133, P0134, P0140, P1133, P2A00, or P2A01 for the 2.4L engine
P0141 | HO2S Heater Performance Sensor 2 | ECM | DTC P0036, P0037, P0038, or P0141 for the 2.0L engine or DTC P0030, P0036, P0053, P0054, P0135, or P0141 for the 2.4L engine
P0171 | Fuel Trim System Lean | ECM | DTC P0171 or P0172 for the 2.4L engine
P0172 | Fuel Trim System Rich | ECM | DTC P0171 or P0172 for the 2.4L engine
P0192 | Fuel Rail Pressure (FRP) Sensor Circuit Low Voltage | ECM | DTC P0192 or P0193 for the 2.0L engine
P0193 | Fuel Rail Pressure (FRP) Sensor Circuit High Voltage | ECM | DTC P0192 or P0193 for the 2.0L engine
P0201 | Injector 1 Control Circuit | ECM | DTC P0201-P0204, P0261, P0262, P0264, P0265, P0267, P0268, P0270, P0271, or P2146-P2157 for the 2.0L engine or DTC P0201, P0202, P0203, or P0204 for the 2.4L engine
P0202 | Injector 2 Control Circuit | ECM | DTC P0201-P0204, P0261, P0262, P0264, P0265, P0267, P0268, P0270, P0271, or P2146-P2157 for the 2.0L engine or DTC P0201, P0202, P0203, or P0204 for the 2.4L engine
P0203 | Injector 3 Control Circuit | ECM | DTC P0201-P0204, P0261, P0262, P0264, P0265, P0267, P0268, P0270, P0271, or P2146-P2157 for the 2.0L engine or DTC P0201, P0202, P0203, or P0204 for the 2.4L engine
P0204 | Injector 4 Control Circuit | ECM | DTC P0201-P0204, P0261, P0262, P0264, P0265, P0267, P0268, P0270, P0271, or P2146-P2157 for the 2.0L engine or DTC P0201, P0202, P0203, or P0204 for the 2.4L engine
P0218 | Transmission Fluid Overtemperature | TCM | DTC P0218
P0220 | Throttle Position (TP) Sensor 2 Circuit | ECM | DTC P0120, P0122, P0123, P0220, P0222, P0223, or P2135 for the 2.4L engine
P0221 | Throttle Position (TP) Sensor 2 Performance | ECM | DTC P0221, P0222, or P0223 for the 2.0L engine
P0222 | Throttle Position (TP) Sensor 2 Circuit Low Voltage | ECM | DTC P0221, P0222, or P0223 for the 2.0L engine or DTC P0120, P0122, P0123, P0220, P0222, P0223, or P2135 for the 2.4L engine
P0223 | Throttle Position (TP) Sensor 2 Circuit High Voltage | ECM | DTC P0221, P0222, or P0223 for the 2.0L engine or DTC P0120, P0122, P0123, P0220, P0222, P0223, or P2135 for the 2.4L engine
P0230 | Fuel Pump Relay Control Circuit | ECM | DTC P0230 for the 2.4L engine
P0234 | Turbocharger Engine Overboost | ECM | DTC P0234 or P0299 for the 2.0L engine
P0236 | Turbocharger Boost System Performance | ECM | DTC P0236, P0237, or P0238 for the 2.0L engine
P0237 | Turbocharger Boost Sensor Circuit Low Voltage | ECM | DTC P0236, P0237, or P0238 for the 2.0L engine
P0238 | Turbocharger Boost Sensor Circuit High Voltage | ECM | DTC P0236, P0237, or P0238 for the 2.0L engine
P0243 | Turbocharger Wastegate Solenoid Control Circuit | ECM | DTC P0243, P0245, or P0246 for the 2.0L engine
P0245 | Turbocharger Wastegate Solenoid Control Circuit Low Voltage | ECM | DTC P0243, P0245, or P0246 for the 2.0L engine
P0246 | Turbocharger Wastegate Solenoid Control Circuit High Voltage | ECM | DTC P0243, P0245, or P0246 for the 2.0L engine
P0261 | Injector 1 Control Circuit Low Voltage | ECM | DTC P0201-P0204, P0261, P0262, P0264, P0265, P0267, P0268, P0270, P0271, or P2146-P2157 for the 2.0L engine
P0262 | Injector 1 Control Circuit High Voltage | ECM | DTC P0201-P0204, P0261, P0262, P0264, P0265, P0267, P0268, P0270, P0271, or P2146-P2157 for the 2.0L engine
P0264 | Injector 2 Control Circuit Low Voltage | ECM | DTC P0201-P0204, P0261, P0262, P0264, P0265, P0267, P0268, P0270, P0271, or P2146-P2157 for the 2.0L engine
P0265 | Injector 2 Control Circuit High Voltage | ECM | DTC P0201-P0204, P0261, P0262, P0264, P0265, P0267, P0268, P0270, P0271, or P2146-P2157 for the 2.0L engine
P0267 | Injector 3 Control Circuit Low Voltage | ECM | DTC P0201-P0204, P0261, P0262, P0264, P0265, P0267, P0268, P0270, P0271, or P2146-P2157 for the 2.0L engine
P0268 | Injector 3 Control Circuit High Voltage | ECM | DTC P0201-P0204, P0261, P0262, P0264, P0265, P0267, P0268, P0270, P0271, or P2146-P2157 for the 2.0L engine
P0270 | Injector 4 Control Circuit Low Voltage | ECM | DTC P0201-P0204, P0261, P0262, P0264, P0265, P0267, P0268, P0270, P0271, or P2146-P2157 for the 2.0L engine
P0271 | Injector 4 Control Circuit High Voltage | ECM | DTC P0201-P0204, P0261, P0262, P0264, P0265, P0267, P0268, P0270, P0271, or P2146-P2157 for the 2.0L engine
P0299 | Turbocharger Engine Underboost | ECM | DTC P0234 or P0299 for the 2.0L engine
P0300 | Engine Misfire Detected | ECM | DTC P0300-P0304 for the 2.0L engine or DTC P0300 for the 2.4L engine
P0301 | Cylinder 1 Misfire Detected | ECM | DTC P0300-P0304 for the 2.0L engine
P0302 | Cylinder 2 Misfire Detected | ECM | DTC P0300-P0304 for the 2.0L engine
P0303 | Cylinder 3 Misfire Detected | ECM | DTC P0300-P0304 for the 2.0L engine
P0304 | Cylinder 4 Misfire Detected | ECM | DTC P0300-P0304 for the 2.0L engine
P0315 | Crankshaft Position (CKP) System Variation Not Learned | ECM | DTC P0315 for the 2.4L engine
P0324 | Knock Sensor (KS) Module Performance | ECM | DTC P0324, P0326, P0327, P0328, P0331, P0332, or P0333 for the 2.0L engine or DTC P0324, P0325, P0326, P0327, or P0328 for the 2.4L engine
P0325 | Knock Sensor (KS) Circuit | ECM | DTC P0324, P0325, P0326, P0327, or P0328 for the 2.4L engine
P0326 | Knock Sensor (KS) 1 Performance | ECM | DTC P0324, P0326, P0327, P0328, P0331, P0332, or P0333 for the 2.0L engine
Knock Sensor (KS) Performance | DTC P0324, P0325, P0326, P0327, or P0328 for the 2.4L engine
P0327 | Knock Sensor (KS) 1 Circuit Low Voltage | ECM | DTC P0324, P0326, P0327, P0328, P0331, P0332, or P0333 for the 2.0L engine
Knock Sensor (KS) Circuit Low Voltage | DTC P0324, P0325, P0326, P0327, or P0328 for the 2.4L engine
P0328 | Knock Sensor (KS) 1 Circuit High Voltage | ECM | DTC P0324, P0326, P0327, P0328, P0331, P0332, or P0333 for the 2.0L engine
Knock Sensor (KS) Circuit High Voltage | DTC P0324, P0325, P0326, P0327, or P0328 for the 2.4L engine
P0331 | Knock Sensor (KS) 2 Performance | ECM | DTC P0324, P0326, P0327, P0328, P0331, P0332, or P0333 for the 2.0L engine
P0332 | Knock Sensor (KS) 2 Circuit Low Voltage | ECM | DTC P0324, P0326, P0327, P0328, P0331, P0332, or P0333 for the 2.0L engine
P0333 | Knock Sensor (KS) 2 Circuit High Voltage | ECM | DTC P0324, P0326, P0327, P0328, P0331, P0332, or P0333 for the 2.0L engine
P0335 | Crankshaft Position (CKP) Sensor Circuit | ECM | DTC P0335, P0336, or P0338 for the 2.0L engine or DTC P0335 or P0336 for the 2.4L engine
P0336 | Crankshaft Position (CKP) Sensor Performance | ECM | DTC P0335, P0336, or P0338 for the 2.0L engine or DTC P0335 or P0336 for the 2.4L engine
P0338 | Crankshaft Position (CKP) Sensor Circuit High Duty Cycle | ECM | DTC P0335, P0336, or P0338 for the 2.0L engine
P0340 | Intake Camshaft Position (CMP) Sensor Circuit | ECM | DTC P0340, P0341, P0365, or P0366 for the 2.4L engine
P0341 | Intake Camshaft Position (CMP) Sensor Performance | ECM | DTC P0341, P0342, or P0343 for the 2.0L engine or DTC P0340, P0341, P0365, or P0366 for the 2.4L engine
P0342 | Intake Camshaft Position (CMP) Sensor Circuit low voltage | ECM | DTC P0341, P0342, or P0343 for the 2.0L engine
P0343 | Intake Camshaft Position (CMP) Sensor Circuit low voltage | ECM | DTC P0341, P0342, or P0343 for the 2.0L engine
P0351 | Ignition Coil 1 Control Circuit | ECM | DTC P0351-P0354 for the 2.4L engine
P0352 | Ignition Coil 2 Control Circuit | ECM | DTC P0351-P0354 for the 2.4L engine
P0353 | Ignition Coil 3 Control Circuit | ECM | DTC P0351-P0354 for the 2.4L engine
P0354 | Ignition Coil 4 Control Circuit | ECM | DTC P0351-P0354 for the 2.4L engine
P0365 | Exhaust Camshaft Position (CMP) Sensor Circuit | ECM | DTC P0340, P0341, P0365, or P0366 for the 2.4L engine
P0366 | Exhaust Camshaft Position (CMP) Sensor Performance | ECM | DTC P0366, P0367, or P0368 for the 2.0L engine or DTC P0340, P0341, P0365, or P0366 for the 2.4L engine
P0367 | Exhaust Camshaft Position (CMP) Sensor Circuit Low Voltage | ECM | DTC P0366, P0367, or P0368 for the 2.0L engine
P0368 | Exhaust Camshaft Position (CMP) Sensor Circuit High Voltage | ECM | DTC P0366, P0367, or P0368 for the 2.0L engine
P0420 | Catalyst System Low Efficiency | ECM | DTC P0420 for the 2.0L engine or DTC P0420 for the 2.4L engine
P0442 | Evaporative Emissions (EVAP) System Small Leak Detected | ECM | DTC P0442 for the 2.0L engine or DTC P0442 for the 2.4L engine
P0443 | Evaporative Emission (EVAP) Purge Solenoid Control Circuit | ECM | DTC P0443, P0449, P0458, P0459, P0498, or P0499 for the 2.0L engine or DTC P0443 or P0449 for the 2.4L engine
P0446 | Evaporative Emissions (EVAP) Vent System Performance | ECM | DTC P0446 for the 2.0L engine or DTC P0446 for the 2.4L engine
P0449 | Evaporative Emission (EVAP) Vent Solenoid Control Circuit | ECM | DTC P0443, P0449, P0458, P0459, P0498, or P0499 for the 2.0L engine or DTC P0443 or P0449 for the 2.4L engine
P0451 | Fuel Tank Pressure (FTP) Sensor Performance | ECM | DTC P0451, P0452, or P0453 for the 2.0L engine or DTC P0451, P0452, P0453, or P0454 for the 2.4L engine
P0452 | Fuel Tank Pressure (FTP) Sensor Circuit Low Voltage | ECM | DTC P0451, P0452, or P0453 for the 2.0L engine or DTC P0451, P0452, P0453, or P0454 for the 2.4L engine
P0453 | Fuel Tank Pressure (FTP) Sensor Circuit High Voltage | ECM | DTC P0451, P0452, or P0453 for the 2.0L engine or DTC P0451, P0452, P0453, or P0454 for the 2.4L engine
P0454 | Fuel Tank Pressure (FTP) Sensor Intermittent | ECM | DTC P0451, P0452, P0453, or P0454 for the 2.4L engine
P0455 | Evaporative Emission (EVAP) System Large Leak | ECM | DTC P0455 for the 2.0L engine or DTC P0455 for the 2.4L engine
P0458 | Evaporative Emission (EVAP) Purge Solenoid Control Circuit Low Voltage | ECM | DTC P0443, P0449, P0458, P0459, P0498, or P0499 for the 2.0L engine
P0459 | Evaporative Emission (EVAP) Purge Solenoid Control Circuit High Voltage | ECM | DTC P0443, P0449, P0458, P0459, P0498, or P0499 for the 2.0L engine
P0461 | Fuel Level Sensor Circuit Performance | ECM | DTC P0461
P0462 | Fuel Level Sensor Circuit Low Voltage | ECM | DTC P0462
P0463 | Fuel Level Sensor Circuit High Voltage | ECM | DTC P0463
P0464 | Fuel Level Sensor 1 Circuit Intermittent | ECM | DTC P0464
P0480 | Cooling Fan Relay 1 Control Circuit | ECM | DTC P0480, P0691, or P0692 for the 2.0L engine or DTC P0480 or P0481 for the 2.4L engine
P0481 | Cooling Fan Relay 2 Control Circuit | ECM | DTC P0480 or P0481 for the 2.4L engine
P0496 | Evaporative Emission System Flow During Non-Purge | ECM | DTC P0496 for the 2.0L engine or DTC P0496 for the 2.4L engine
P0498 | Evaporative Emission (EVAP) Vent Solenoid Control Circuit Low Voltage | ECM | DTC P0443, P0449, P0458, P0459, P0498, or P0499 for the 2.0L engine
P0499 | Evaporative Emission (EVAP) Vent Solenoid Control Circuit High Voltage | ECM | DTC P0443, P0449, P0458, P0459, P0498, or P0499 for the 2.0L engine
P0500 | Vehicle Speed Sensor (VSS) Circuit | TCM | DTC P0500
P0502 | Vehicle Speed Sensor (VSS) Circuit Low Voltage | ECM | DTC P0502
P0503 | Vehicle Speed Sensor (VSS) Circuit Intermittent | ECM | DTC P0503
P0506 | Idle Speed Low | ECM | DTC P0506 or P0507 for the 2.0L engine or DTC P0506 or P0507 for the 2.4L engine
P0507 | Idle Speed High | ECM | DTC P0506 or P0507 for the 2.0L engine or DTC P0506 or P0507 for the 2.4L engine
P050A | Cold Start Idle Air Control System Performance | ECM | DTC P050A for the 2.0L engine
P0520 | Engine Oil Pressure (EOP) Sensor Circuit | ECM | DTC P0520
P0532 | Air Conditioning (A/C) Refrigerant Pressure Sensor Circuit Low Voltage | ECM | DTC P0532 or P0533
P0533 | Air Conditioning (A/C) Refrigerant Pressure Sensor Circuit High Voltage | ECM | DTC P0532 or P0533
P0556 | Brake Booster Pressure Sensor Performance | ECM | DTC P0556
P0557 | Brake Booster Pressure Sensor Circuit Low Voltage | ECM | DTC P0557
P0558 | Brake Booster Pressure Sensor Circuit High Voltage | ECM | DTC P0558
P0560 | System Voltage | ECM | DTC P0560
P0562 | System Voltage Low | ECM | DTC P0562
TCM | DTC P0562
P0563 | System Voltage High | ECM | DTC P0563
TCM | DTC P0563
P0571 | Cruise Control Brake Switch Circuit | ECM | DTC P0571
P0572 | Brake Switch Circuit 1 Low Voltage | ECM | DTC P0572
P0573 | Brake Switch Circuit 1 High Voltage | ECM | DTC P0573
P0575 | Cruise Control Switch Signal Circuit | ECM | DTC P0575
P0601 | Control Module Read Only Memory (ROM) | ECM | DTC P0601, P0602, P0603, P0604, P0606, P062B, P167A, P167D, P2105, P2107, or P2610 for the 2.0L engine or DTC P0601, P0602, P0603, P0604, P0606, P0607, P060D, P062F, or P2610 for the 2.4L engine
Transmission Control Module (TCM) Read Only Memory (ROM) | TCM | DTC P0601-P0604 or P062F
P0602 | Control Module Not Programmed | ECM | DTC P0601, P0602, P0603, P0604, P0606, P062B, P167A, P167D, P2105, P2107, or P2610 for the 2.0L engine or DTC P0601, P0602, P0603, P0604, P0606, P0607, P060D, P062F, or P2610 for the 2.4L engine
Transmission Control Module (TCM) Not Programmed | TCM | DTC P0601-P0604 or P062F
P0603 | Control Module Long Term Memory Reset | ECM | DTC P0601, P0602, P0603, P0604, P0606, P062B, P167A, P167D, P2105, P2107, or P2610 for the 2.0L engine or DTC P0601, P0602, P0603, P0604, P0606, P0607, P060D, P062F, or P2610 for the 2.4L engine
Transmission Control Module (TCM) Long Term Memory Reset | TCM | DTC P0601-P0604 or P062F
P0604 | Control Module Random Access Memory (RAM) | ECM | DTC P0601, P0602, P0603, P0604, P0606, P062B, P167A, P167D, P2105, P2107, or P2610 for the 2.0L engine or DTC P0601, P0602, P0603, P0604, P0606, P0607, P060D, P062F, or P2610 for the 2.4L engine
Transmission Control Module (TCM) Random Access Memory (RAM) | TCM | DTC P0601-P0604 or P062F
P0606 | Control Module Internal Performance | ECM | DTC P0601, P0602, P0603, P0604, P0606, P062B, P167A, P167D, P2105, P2107, or P2610 for the 2.0L engine or DTC P0601, P0602, P0603, P0604, P0606, P0607, P060D, P062F, or P2610
P0607 | Control Module Performance | ECM | DTC P0601, P0602, P0603, P0604, P0606, P0607, P060D, P062F, or P2610 for the 2.4L engine
P060D | Control Module Accelerator Pedal Position (APP) System Performance | ECM | DTC P0601, P0602, P0603, P0604, P0606, P0607, P060D, P062F, or P2610 for the 2.4L engine
P0615 | Starter Relay Control Circuit | ECM | DTC P0615
P0616 | Starter Relay Control Circuit Low Voltage | ECM | DTC P0616
P0617 | Starter Relay Control Circuit High Voltage | ECM | DTC P0617
P0621 | Generator L-Terminal Circuit | ECM | DTC P0621
P0622 | Generator F-Terminal Circuit | ECM | DTC P0622
P0626 | Generator F-Terminal Circuit High Voltage | ECM | DTC P0626
P0627 | Fuel Pump Relay Control Circuit | ECM | DTC P0627, P0628, or P0629 for the 2.0L engine
P0628 | Fuel Pump Relay Control Circuit Low Voltage | ECM | DTC P0627, P0628, or P0629 for the 2.0L engine
P0629 | Fuel Pump Relay Control Circuit High Voltage | ECM | DTC P0627, P0628, or P0629 for the 2.0L engine
P062B | Control Module Fuel Injector Control Performance | ECM | DTC P0601, P0602, P0603, P0604, P0606, P062B, P167A, P167D, P2105, P2107, or P2610 for the 2.0L engine
P062F | Control Module Long Term Memory Performance | ECM | DTC P0601, P0602, P0603, P0604, P0606, P0607, P060D, P062F, or P2610 for the 2.4L engine
Transmission Control Module (TCM) Long Term Memory Performance | TCM | DTC P0601-P0604 or P062F
P0638 | Throttle Actuator Control (TAC) Command Performance | ECM | DTC P0638, P1551, P2100, P2101, P2119, or P2176 for the 2.0L engine
P0641 | 5-Volt Reference 1 Circuit | ECM | DTC P0641, P0642, P0643, P0651, P0652, P0653, P0697, P0698 or P0699 for the 2.0L engine or DTC P0641 or P0651 for the 2.4L engine
P0642 | 5-Volt Reference 1 Low Voltage | ECM | DTC P0641, P0642, P0643, P0651, P0652, P0653, P0697, P0698 or P0699 for the 2.0L engine
P0643 | 5-Volt Reference 1 High Voltage | ECM | DTC P0641, P0642, P0643, P0651, P0652, P0653, P0697, P0698 or P0699 for the 2.0L engine
P0645 | Air Conditioning (A/C) Clutch Relay Control Circuit | ECM | DTC P0645
P0650 | Malfunction Indicator Lamp (MIL) Control Circuit | ECM | DTC P0650 for the 2.0L engine or DTC P0650 for the 2.4L engine
P0651 | 5-Volt Reference 2 Circuit | ECM | DTC P0641, P0642, P0643, P0651, P0652, P0653, P0697, P0698 or P0699 for the 2.0L engine or DTC P0641 or P0651 for the 2.4L engine
P0652 | 5-Volt Reference 2 Low Voltage | ECM | DTC P0641, P0642, P0643, P0651, P0652, P0653, P0697, P0698 or P0699 for the 2.0L engine
P0653 | 5-Volt Reference 2 High Voltage | ECM | DTC P0641, P0642, P0643, P0651, P0652, P0653, P0697, P0698 or P0699 for the 2.0L engine
P0685 | Engine Controls Ignition Relay Control Circuit | ECM | DTC P0685, P0686, P0687, P0689, or P0690 for the 2.0L engine or DTC P0685, P0689, or P0690 for the 2.4L engine
P0686 | Engine Controls Ignition Relay Control Circuit Low Voltage | ECM | DTC P0685, P0686, P0687, P0689, or P0690 for the 2.0L engine
P0687 | Engine Controls Ignition Relay Control Circuit High Voltage | ECM | DTC P0685, P0686, P0687, P0689, or P0690 for the 2.0L engine
P0689 | Engine Controls Ignition Relay Feedback Circuit Low Voltage | ECM | DTC P0685, P0686, P0687, P0689, or P0690 for the 2.0L engine or DTC P0685, P0689, or P0690 for the 2.4L engine
P0690 | Engine Controls Ignition Relay Feedback Circuit High Voltage | ECM | DTC P0685, P0686, P0687, P0689, or P0690 for the 2.0L engine or DTC P0685, P0689, or P0690 for the 2.4L engine
P0691 | Cooling Fan Speed Output Circuit Low Voltage | ECM | DTC P0480, P0691, or P0692
P0692 | Cooling Fan Speed Output Circuit High Voltage | ECM | DTC P0480, P0691, or P0692
P0697 | 5-Volt Reference 3 Circuit | ECM | DTC P0641, P0642, P0643, P0651, P0652, P0653, P0697, P0698 or P0699 for the 2.0L engine
P0698 | 5-Volt Reference 3 Low Voltage | ECM | DTC P0641, P0642, P0643, P0651, P0652, P0653, P0697, P0698 or P0699 for the 2.0L engine
P0699 | 5-Volt Reference 3 High Voltage | ECM | DTC P0641, P0642, P0643, P0651, P0652, P0653, P0697, P0698 or P0699 for the 2.0L engine
P0700 | Transmission Control Module (TCM) Requested MIL Illumination | ECM | DTC P0700 for the 2.0L engine or DTC P0700 or P1700 for the 2.4L engine
P0703 | Brake Switch Circuit 2 | ECM | DTC P0703
P0711 | Transmission Fluid Temperature (TFT) Sensor Performance | TCM | DTC P0711
P0712 | Transmission Fluid Temperature (TFT) Sensor Circuit Low Voltage | TCM | DTC P0712
P0713 | Transmission Fluid Temperature (TFT) Sensor Circuit High Voltage | TCM | DTC P0713
P0716 | Input Speed Sensor Performance | TCM | DTC P0716
P0717 | Input Speed Sensor Circuit Low Voltage | TCM | DTC P0717
P0722 | Output Speed Sensor Circuit Low Voltage | TCM | DTC P0722
P0723 | Output Speed Sensor Circuit Intermittent | TCM | DTC P0723
P0727 | Engine Speed No Signal | TCM | DTC P0727
P0741 | Torque Converter Clutch (TCC) System - Stuck Off | TCM | DTC P0741
P0742 | Torque Converter Clutch (TCC) System - Stuck On | TCM | DTC P0742
P0748 | Pressure Control (PC) Solenoid Control Circuit | TCM | DTC P0748
P0751 | 1-2 Shift Solenoid (SS) Valve Performance - No First, Fourth or Fifth Gear | TCM | DTC P0751
P0752 | 1-2 Shift Solenoid (SS) Valve Performance - No Second or Third Gear | TCM | DTC P0752
P0756 | 2-3 Shift Solenoid (SS) Valve Performance - No First or Second Gear | TCM | DTC P0756
P0757 | 2-3 Shift Solenoid (SS) Valve Performance - No Third, Fourth or Fifth Gear | TCM | DTC P0757
P0761 | 4-5 Shift Solenoid (SS) Valve Performance - No Fourth Gear | TCM | DTC P0761
P0762 | 4-5 Shift Solenoid (SS) Valve Performance - No Fifth Gear | TCM | DTC P0762
P0833 | Clutch Pedal Switch 2 Circuit | ECM | DTC P0833
P0850 | Park/Neutral Position (PNP) Switch Circuit | TCM | DTC P0850
P0973 | 1-2 Shift Solenoid (SS) Control Circuit Low Voltage | TCM | DTC P0973
P0974 | 1-2 Shift Solenoid (SS) Control Circuit High Voltage | TCM | DTC P0974
P0976 | 2-3 Shift Solenoid (SS) Control Circuit Low Voltage | TCM | DTC P0976
P0977 | 2-3 Shift Solenoid (SS) Control Circuit High Voltage | TCM | DTC P0977
P0979 | 4-5 Shift Solenoid (SS) Control Circuit Low Voltage | TCM | DTC P0979
P0980 | 4-5 Shift Solenoid (SS) Control Circuit High Voltage | TCM | DTC P0980
P1011 | Intake Camshaft Position (CMP) Actuator Park Position Circuit | ECM | DTC P1011 for the 2.0L engine
P1012 | Intake Camshaft Position (CMP) Actuator Park Position Circuit | ECM | DTC P1012 for the 2.0L engine
P1101 | Intake Air Flow System Performance | ECM | DTC P0101 or P1101 for the 2.4L engine
P1133 | HO2S Insufficient Switching Sensor 1 | ECM | DTC P0133, P0134, P0140, P1133, P2A00, or P2A01 for the 2.4L engine
P1174 | Fuel Trim Cylinder Balance | ECM | DTC P1174
P1400 | Cold Start Emission Reduction Control System | ECM | DTC P1400
P1516 | Throttle Actuator Control (TAC) Module Throttle Actuator Position Performance | ECM | DTC P1516, P2101, P2119, or P2176
P1551 | Throttle Valve Rest Position Not Reached During Learn | ECM | DTC P0638, P1551, P2100, P2101, P2119, or P2176 for the 2.0L engine
P1629 | Theft Deterrent Fuel Enable Signal Not Received | ECM | DTC P1629
P1631 | Theft Deterrent Fuel Enable Signal Not Correct | ECM | DTC P1631
P1632 | Theft Deterrent Start Disable Signal Received | ECM | DTC P1632
P167A | Control Module HO2S 1 System Performance | ECM | DTC P0601, P0602, P0603, P0604, P0606, P062B, P167A, P167D, P2105, P2107, or P2610 for the 2.0L engine
P167D | Control Module Ignition Coil Internal Circuit | ECM | DTC P0601, P0602, P0603, P0604, P0606, P062B, P167A, P167D, P2105, P2107, or P2610 for the 2.0L engine
P1682 | Ignition 1 Switch Circuit 2 | ECM | DTC P1682
P1793 | Wheel Speed Signal | TCM | DTC P1793
P1820 | Internal Mode Switch A Circuit Low Voltage | TCM | DTC P1820
P1822 | Internal Mode Switch B Circuit High Voltage | TCM | DTC P1822
P1823 | Internal Mode Switch P Circuit Low Voltage | TCM | DTC P1823
P1825 | Internal Mode Switch - Invalid Range | TCM | DTC P1825
P1826 | Internal Mode Switch C Circuit High Voltage | TCM | DTC P1826
P1831 | Pressure Control (PC)/Shift Lock Solenoid Control Circuit Low Voltage | TCM | DTC P1831
P1832 | Pressure Control (PC)/Shift Lock Solenoid Control Circuit High Voltage | TCM | DTC P1832
P1833 | Torque Converter Clutch (TCC)/Shift Solenoid (SS) Control Circuit Low Voltage | TCM | DTC P1833
P1834 | Torque Converter Clutch (TCC)/Shift Solenoid (SS) Control Circuit High Voltage | TCM | DTC P1834
P1915 | Internal Mode Switch Does Not Indicate Park/Neutral (P/N) During Start | TCM | DTC P1915
P2088 | Intake Camshaft Position (CMP) Actuator Solenoid Control Circuit Low Voltage | ECM | DTC P2088 or P2089 for the 2.0L engine
P2089 | Intake Camshaft Position (CMP) Actuator Solenoid Control Circuit High Voltage | ECM | DTC P2088 or P2089 for the 2.0L engine
P2090 | Exhaust Camshaft Position (CMP) Actuator Solenoid Control Circuit Low Voltage | ECM | DTC P2090 or P2091 for the 2.0L engine
P2091 | Exhaust Camshaft Position (CMP) Actuator Solenoid Control Circuit High Voltage | ECM | DTC P2090 or P2091 for the 2.0L engine
P2096 | Post Catalyst Fuel Trim System Low Limit Bank 1 | ECM | DTC P2096 for the 2.0L engine
P2097 | Post Catalyst Fuel Trim System High Limit Bank 1 | ECM | DTC P2097 for the 2.0L engine
P2100 | Throttle Actuator Control (TAC) Motor Control Circuit | ECM | DTC P0638, P1551, P2100, P2101, P2119, or P2176 for the 2.0L engine
P2101 | Control Module Throttle Actuator Position Performance | ECM | DTC P0638, P1551, P2100, P2101, P2119, or P2176 for the 2.0L engine or DTC P1516, P2101, P2119, or P2176 for the 2.4L engine.
P2105 | Throttle Actuator Control (TAC) System - Forced Engine Shut-down | ECM | DTC P0601, P0602, P0603, P0604, P0606, P062B, P167A, P167D, P2105, P2107, or P2610 for the 2.0L engine
P2107 | Throttle Actuator Control (TAC) Module Internal Circuit | ECM | DTC P0601, P0602, P0603, P0604, P0606, P062B, P167A, P167D, P2105, P2107, or P2610 for the 2.0L engine
P2119 | Throttle Closed Position Performance | ECM | DTC P0638, P1551, P2100, P2101, P2119, or P2176 for the 2.0L engine or DTC P1516, P2101, P2119, or P2176 for the 2.4L engine
P2120 | Accelerator Pedal Position (APP) Sensor 1 Circuit | ECM | DTC P2120, P2122, P2123, P2125, P2127, P2128, or P2138 for the 2.4L engine
P2122 | Accelerator Pedal Position (APP) Sensor 1 Circuit Low Voltage | ECM | DTC P2122 or P2123 for the 2.0L engine or DTC P2120, P2122, P2123, P2125, P2127, P2128, or P2138 for the 2.4L engine
P2123 | Accelerator Pedal Position (APP) Sensor 1 Circuit High Voltage | ECM | DTC P2122 or P2123 for the 2.0L engine or DTC P2120, P2122, P2123, P2125, P2127, P2128, or P2138 for the 2.4L engine
P2125 | Accelerator Pedal Position (APP) Sensor 2 Circuit | ECM | DTC P2120, P2122, P2123, P2125, P2127, P2128, or P2138 for the 2.4L engine
P2127 | Accelerator Pedal Position (APP) Sensor 2 Circuit Low Voltage | ECM | DTC P2127 or P2128 for the 2.0L engine or DTC P2120, P2122, P2123, P2125, P2127, P2128, or P2138 for the 2.4L engine
P2128 | Accelerator Pedal Position (APP) Sensor 2 Circuit High Voltage | ECM | DTC P2127 or P2128 for the 2.0L engine or DTC P2120, P2122, P2123, P2125, P2127, P2128, or P2138 for the 2.4L engine
P2135 | Throttle Position (TP) Sensor 1-2 Correlation | ECM | DTC P0120, P0122, P0123, P0220, P0222, P0223, or P2135 for the 2.4L engine
P2138 | Accelerator Pedal Position (APP) Sensor 1-2 Correlation | ECM | DTC P2138 for the 2.0L engine or DTC P2120, P2122, P2123, P2125, P2127, P2128, or P2138 for the 2.4L engine
P2146 | Injector Positive Voltage Control Circuit Group 1 | ECM | DTC P0201-P0204, P0261, P0262, P0264, P0265, P0267, P0268, P0270, P0271, or P2146-P2157 for the 2.0L engine
P2147 | Injector Positive Voltage Control Circuit Group 1 Low Voltage | ECM | DTC P0201-P0204, P0261, P0262, P0264, P0265, P0267, P0268, P0270, P0271, or P2146-P2157 for the 2.0L engine
P2148 | Injector Positive Voltage Control Circuit Group 1 High Voltage | ECM | DTC P0201-P0204, P0261, P0262, P0264, P0265, P0267, P0268, P0270, P0271, or P2146-P2157 for the 2.0L engine
P2149 | Injector Positive Voltage Control Circuit Group 2 | ECM | DTC P0201-P0204, P0261, P0262, P0264, P0265, P0267, P0268, P0270, P0271, or P2146-P2157 for the 2.0L engine
P2150 | Injector Positive Voltage Control Circuit Group 2 Low Voltage | ECM | DTC P0201-P0204, P0261, P0262, P0264, P0265, P0267, P0268, P0270, P0271, or P2146-P2157 for the 2.0L engine
P2151 | Injector Positive Voltage Control Circuit Group 2 High Voltage | ECM | DTC P0201-P0204, P0261, P0262, P0264, P0265, P0267, P0268, P0270, P0271, or P2146-P2157 for the 2.0L engine
P2152 | Injector Positive Voltage Control Circuit Group 3 | ECM | DTC P0201-P0204, P0261, P0262, P0264, P0265, P0267, P0268, P0270, P0271, or P2146-P2157 for the 2.0L engine
P2153 | Injector Positive Voltage Control Circuit Group 3 Low Voltage | ECM | DTC P0201-P0204, P0261, P0262, P0264, P0265, P0267, P0268, P0270, P0271, or P2146-P2157 for the 2.0L engine
P2154 | Injector Positive Voltage Control Circuit Group 3 High Voltage | ECM | DTC P0201-P0204, P0261, P0262, P0264, P0265, P0267, P0268, P0270, P0271, or P2146-P2157 for the 2.0L engine
P2155 | Injector Positive Voltage Control Circuit Group 4 | ECM | DTC P0201-P0204, P0261, P0262, P0264, P0265, P0267, P0268, P0270, P0271, or P2146-P2157 for the 2.0L engine
P2156 | Injector Positive Voltage Control Circuit Group 4 Low Voltage | ECM | DTC P0201-P0204, P0261, P0262, P0264, P0265, P0267, P0268, P0270, P0271, or P2146-P2157 for the 2.0L engine
P2157 | Injector Positive Voltage Control Circuit Group 4 High Voltage | ECM | DTC P0201-P0204, P0261, P0262, P0264, P0265, P0267, P0268, P0270, P0271, or P2146-P2157 for the 2.0L engine
P2176 | Minimum Throttle Position Not Learned | ECM | DTC P0638, P1551, P2100, P2101, P2119, or P2176 for the 2.0L engine or DTC P1516, P2101, P2119, or P2176 for the 2.4L engine
P2177 | Fuel Trim System Lean at Cruise or Accel | ECM | DTC P2177 or P2187 for the 2.0L engine
P2178 | Fuel Trim System Rich at Cruise or Accel | ECM | DTC P2178 or P2188 for the 2.0L engine
P2187 | Fuel Trim System Lean at Idle | ECM | DTC P2177 or P2187 for the 2.0L engine
P2188 | Fuel Trim System Rich at Idle | ECM | DTC P2178 or P2188 for the 2.0L engine
P2195 | HO2S Signal Biased Lean Sensor 1 | ECM | DTC P0130, P0131, P0132, P0133, P2195, P2196, P2231, or P2297 for the 2.0L engine
P2196 | HO2S Signal Biased Rich Sensor 1 | ECM | DTC P0130, P0131, P0132, P0133, P2195, P2196, P2231, or P2297 for the 2.0L engine
P2199 | Intake Air Temperature (IAT) Sensor 1-2 Correlation | ECM | DTC P2199 for the 2.0L engine
P2227 | Barometric Pressure (BARO) Sensor Performance | ECM | DTC P2227, P2228, or P2229 for the 2.0L engine
P2228 | Barometric Pressure (BARO) Sensor Circuit Low Voltage | ECM | DTC P2227, P2228, or P2229 for the 2.0L engine
P2229 | Barometric Pressure (BARO) Sensor Circuit High Voltage | ECM | DTC P2227, P2228, or P2229 for the 2.0L engine
P2231 | HO2S Signal Circuit Shorted to Heater Circuit Sensor 1 | ECM | DTC P0130, P0131, P0132, P0133, P2195, P2196, P2231, or P2297 for the 2.0L engine
P2232 | HO2S Signal Circuit Shorted to Heater Circuit Sensor 2 | ECM | DTC P0137, P0138, P0139, P0140, P2232, P2270, or P2271 for the 2.0L engine
P2237 | HO2S Pumping Current Control Circuit Sensor 1 | ECM | DTC P2237, P2243, P2251, or P2626 for the 2.0L engine
P2243 | HO2S Reference Voltage Circuit Sensor 1 | ECM | DTC P2237, P2243, P2251, or P2626 for the 2.0L engine
P2251 | HO2S Low Reference Circuit Sensor 1 | ECM | DTC P2237, P2243, P2251, or P2626 for the 2.0L engine
P2261 | Turbocharger Bypass Valve Stuck | ECM | DTC P2261 for the 2.0L engine
P2270 | HO2S Signal Stuck Lean Sensor 2 | ECM | DTC P0137, P0138, P0139, P0140, P2232, P2270, or P2271 for the 2.0L engine
P2271 | HO2S Signal Stuck Rich Sensor 2 | ECM | DTC P0137, P0138, P0139, P0140, P2232, P2270, or P2271 for the 2.0L engine
P2297 | HO2S Performance During Decel Fuel Cut-Off (DFCO) Sensor 1 | ECM | DTC P0130, P0131, P0132, P0133, P2195, P2196, P2231, or P2297 for the 2.0L engine
P2300 | Ignition Coil 1 Control Circuit Low Voltage | ECM | DTC P2300, P2301, P2303, P2304, P2306, P2307, P2309, or P2310 for the 2.0L engine
P2301 | Ignition Coil 1 Control Circuit High Voltage | ECM | DTC P2300, P2301, P2303, P2304, P2306, P2307, P2309, or P2310 for the 2.0L engine
P2303 | Ignition Coil 2 Control Circuit Low Voltage | ECM | DTC P2300, P2301, P2303, P2304, P2306, P2307, P2309, or P2310 for the 2.0L engine
P2304 | Ignition Coil 2 Control Circuit High Voltage | ECM | DTC P2300, P2301, P2303, P2304, P2306, P2307, P2309, or P2310 for the 2.0L engine
P2306 | Ignition Coil 3 Control Circuit Low Voltage | ECM | DTC P2300, P2301, P2303, P2304, P2306, P2307, P2309, or P2310 for the 2.0L engine
P2307 | Ignition Coil 3 Control Circuit High Voltage | ECM | DTC P2300, P2301, P2303, P2304, P2306, P2307, P2309, or P2310 for the 2.0L engine
P2309 | Ignition Coil 4 Control Circuit Low Voltage | ECM | DTC P2300, P2301, P2303, P2304, P2306, P2307, P2309, or P2310 for the 2.0L engine
P2310 | Ignition Coil 4 Control Circuit High Voltage | ECM | DTC P2300, P2301, P2303, P2304, P2306, P2307, P2309, or P2310 for the 2.0L engine
P2500 | Generator L-Terminal Circuit Low Voltage | ECM | DTC P2500
P2501 | Generator L-Terminal Circuit High Voltage | ECM | DTC P2501
P2535 | Ignition 1 Switch Circuit High Voltage | ECM | DTC P2535
P2544 | Transmission Torque Request Circuit | TCM |

• | DTC P2544 for the 2.0L engine

• | DTC P2544 for the 2.4L engine

• | DTC P2544 for the 5L40-E/5L50-E transmission

P258A | Vacuum Pump Relay Control Circuit | ECM | DTC P258A-P258D
P258B | Vacuum Pump Performance | ECM | DTC P258A-P258D
P258C | Vacuum Pump Relay Control Circuit Low Voltage | ECM | DTC P258A-P258D
P258D | Vacuum Pump Relay Control Circuit High Voltage | ECM | DTC P258A-P258D
P2610 | Control Module Ignition Off Timer Performance | ECM | DTC P0601, P0602, P0603, P0604, P0606, P062B, P167A, P167D, P2105, P2107, or P2610 for the 2.0L engine or DTC P0601, P0602, P0603, P0604, P0606, P0607, P060D, P062F, or P2610 for the 2.4L engine
P2626 | HO2S Pumping Current Trim Circuit Sensor 1 | ECM | DTC P2237, P2243, P2251, or P2626 for the 2.0L engine
P2637 | Transmission Torque Delivered Circuit | TCM | DTC P2637
P2763 | Torque Converter Clutch (TCC) Pressure Control (PC) Solenoid Control Circuit High Voltage | TCM | DTC P2763
P2764 | Torque Converter Clutch (TCC) Pressure Control (PC) Solenoid Control Circuit Low Voltage | TCM | DTC P2764
P2A00 | HO2S Circuit Closed Loop (CL) Performance Sensor 1 | ECM | DTC P0133, P0134, P0140, P1133, P2A00, or P2A01 for the 2.4L engine
P2A01 | HO2S Circuit Sensor 2 | ECM | DTC P0133, P0134, P0140, P1133, P2A00, or P2A01 for the 2.4L engine
U0001 | High Speed CAN Communication Bus | ECM, RCDLR | DTC U0001
U0020 | Low Speed CAN Communication Bus Performance | Radio, | DTC U0020
U0073 | Controller Area Network (CAN) Bus Communication | ECM, Radio, RCDLR | DTC U0073 or U2100
U0100 | Lost Communication With Engine Control Module (ECM) | TCM | DTC U0100-U0299 or U2105-U2199
U0101 | Lost Communication With Transmission Control Module (TCM) | ECM | DTC U0100-U0299 or U2105-U2199
U0121 | Lost Communication With Antilock Brake Module (ABS) | ECM | DTC U0100-U0299 or U2105-U2199
U0140 | Lost Communication With Body Control Module (BCM) | ECM | DTC U0100-U0299 or U2105-U2199
U2100 | Controller Area Network (CAN) Bus Communication | BCM, DRR, EBCM, IPC, RCDLR, SDM, TDM, VCIM | DTC U0073 or U2100
U2103 | Fewer Controllers On Bus Than Programmed | BCM, DRR, IPC, SDM, VCIM | DTC U2103
U2105 | Lost Communications With Engine Control System | BCM, EBCM, TDM | DTC U0100-U0299 or U2105-U2199
U2106 | Lost Communications With Transmission Control System | BCM, EBCM | DTC U0100-U0299 or U2105-U2199
U2107 | Lost Communications With Body Control System | EBCM, IPC, RCDLR, TDM | DTC U0100-U0299 or U2105-U2199
U2108 | Lost Communications With ABS/TCS Control System | BCM | DTC U0100-U0299 or U2105-U2199
U2111 | Lost Communications With Steering Control System | BCM | DTC U0100-U0299 or U2105-U2199
U2113 | Lost Communications With Sensing Diagnostic Module (SDM) | BCM | DTC U0100-U0299 or U2105-U2199
U2116 | Lost Communications With Instrument Panel Cluster (IPC) | BCM | DTC U0100-U0299 or U2105-U2199
U2122 | Lost Communications With Radio | BCM | DTC U0100-U0299 or U2105-U2199
U2125 | Lost Communication With Mobile Communications Control Systems | BCM | DTC U0100-U0299 or U2105-U2199
U2137 | Lost Communications With Vehicle Theft Deterrent (VTD) | BCM | DTC U0100-U0299 or U2105-U2199
U2171 | Lost Communications With DVD Player | BCM | DTC U0100-U0299 or U2105-U2199
U2172 | Lost Communications With Digital Radio Receiver | BCM | DTC U0100-U0299 or U2105-U2199
1049-1050 | PPS System Fault | PPS | DTC 1049-1050
1051 | PPS Initialization/Preload Fault | PPS | DTC 1051
1052 | PPS Preload Failure Region 1 | PPS | DTC 1052, 1053, 1054, or 1055
1053 | PPS Preload Failure Region 2 | PPS | DTC 1052, 1053, 1054, or 1055
1054 | PPS Preload Failure Region 3 | PPS | DTC 1052, 1053, 1054, or 1055
1055 | PPS Preload Failure Region 4 | PPS | DTC 1052, 1053, 1054, or 1055
1058-1062 | PPS Communication Fault | PPS | DTC 1058-1062
1063 | Discard System | PPS | DTC 1063
2036-2045 | Internal Electronic Performance 2 | PPS | DTC 2036-2045
3011-3035 | Internal Electronic Performance 1 | PPS | DTC 3011-3035