For 1990-2009 cars

### Removal Procedure

1. Disconnect the engine wiring harness electrical connector (2) from the manifold absolute pressure (MAP) sensor.
2. Remove the MAP sensor bolts.
3. Remove the MAP sensor and O-ring seal from the intake manifold.

### Installation Procedure

1. Lubricate the O-ring seal with clean engine oil.
2. Install the MAP sensor to the intake manifold.

Caution: Refer to Fastener Caution in the Preface section.

3. Install the MAP sensor bolts and tighten to 10 N·m (89 lb in).
4. Connect the engine wiring harness electrical connector (2) to the MAP sensor.