For 1990-2009 cars

## Windshield Washer Solvent Container Hose Replacement SKY

Callout | Component Name
--- | ---

#### Preliminary Procedures

1. Open the hood.
2. Disconnect the washer hose at the driver side hinge pillar to air inlet grille panel.
3. Disconnect the washer hose retention clip.
4. Remove the left front wheelhouse liner. Refer to Front Wheelhouse Liner Replacement .
5. Remove the washer hose from the washer pump spout.
6. Drain the washer solvent into a suitable container.
7. Disconnect the hose from the washer container.

1 | Windshield Washer Pump Hose to Air Inlet Grille Panel Hose Connection
2 | Washer Hose Retention Clip
3 | Washer Solvent Container to Washer Pump Hose Tip Ensure the washer hose is re-routed properly to the washer solvent container and secured.

## Windshield Washer Solvent Container Hose Replacement Solstice

Callout | Component Name
--- | ---

#### Preliminary Procedures

1. Open the hood.
2. Disconnect the washer hose at the driver side hinge pillar to air inlet grille panel.
3. Disconnect the washer hose retention clip.
4. Remove the left front wheelhouse liner. Refer to Front Wheelhouse Liner Replacement .
5. Remove the washer hose from the washer pump spout.
6. Drain the washer solvent into a suitable container.
7. Disconnect the hose from the washer container.

1 | Windshield Washer Pump Hose to Air Inlet Grille Panel Hose Connection
2 | Washer Hose Retention Clip
3 | Washer Solvent Container to Washer Pump Hose Tip Ensure the washer hose is re-routed properly to the washer solvent container and secured.