For 1990-2009 cars

#### Tools Required

J 42067 Rear Main Seal Installer

### Removal Procedure

1. Remove the flywheel. Refer to Engine Flywheel Replacement .

Important: Do not damage the outside diameter of the crankshaft or chamber with any tool.

2. Pry out the crankshaft rear oil seal using a flat-bladed tool.

### Installation Procedure

1. Using the J 42067 , install a NEW crankshaft real oil seal.
2. Install the flywheel. Refer to Engine Flywheel Replacement .