For 1990-2009 cars

## Front Fender Emblem/Nameplate Replacement Solstice

Callout | Component Name
--- | ---
1 | Front Fender Emblem Tip

1. Clean the adhesive tape residue from the surface of the front fender and dry thoroughly before applying the new emblem.
2. Peel protective backing from emblem and ensure no foreign matter or dirt comes in contact with the adhesive backing prior to installation.
3. Install the emblem and apply pressure to ensure full adhesion is made to the front fender.