For 1990-2009 cars

Callout | Component Name
--- | ---
1 | Roof Lift Off Panel Rear Latch Striker Fastener (Qty: 2) Caution: Refer to Fastener Caution in the Preface section.

#### Procedure

1. Place the roof panel on a protective surface.
2. Remove the latch striker cover.
3. Using a marker to mark the location of the latch striker before removing it.

Tighten
Tighten the fastener to 10 N·m (89 lb in).

2 | Roof Lift Off Panel Rear Latch Striker

#### Procedure

Rear latch striker. Refer to Roof Lift Off Panel Adjustment