For 1990-2009 cars

Callout | Component Name
--- | ---
Notice: Refer to Fastener Notice in the Preface section. Fastener Tightening Specifications: Refer to Fastener Tightening Specifications .

#### Preliminary Procedures

1. Remove the rear bumper fascia. Refer to Rear Bumper Fascia Replacement .
2. Remove the two lower back up lamp screws from the rear bumper valance center panel.

1 | Back Up Lamp Assembly Screws (Qty: 4) Tighten 2 N·m (18 lb in)
2 | Back Up Lamp Assembly Tip Replace the lamp bulb, if needed.