For 1990-2009 cars

## Instrument Panel Tie Bar Replacement Sky

Callout | Component Name
--- | ---

#### Preliminary Procedures

1. Remove the instrument panel (I/P) carrier assembly. Refer to Instrument Panel Carrier Replacement.
2. Note the routing of the I/P wiring harness around the I/P tie bar to ensure the proper reinstallation.
3. Remove the nuts securing the air distribution duct to the I/P tie bar. Refer to Air Distributor Duct Replacement.
4. Remove the bolts securing the I/P tie bar to the brake pedal bracket.

1 | I/P Tie Bar Bolt (Qty: 4) Caution: Refer to Fastener Caution in the Preface section. Tighten 25 N·m (18 lb ft)
2 | I/P Tie Bar Bolt (Qty: 2) Tighten 58 N·m (34 lb ft)
3 | I/P Tie Bar Assembly

#### Procedure

With the aid of an assistant, remove the tie bar from the vehicle.

## Instrument Panel Tie Bar Replacement Solstice

Callout | Component Name
--- | ---

#### Preliminary Procedures

1. Remove the instrument panel (I/P) carrier assembly. Refer to Instrument Panel Carrier Replacement.
2. Note the routing of the I/P wiring harness around the I/P tie bar to aid in the reinstallation procedure.
3. Remove the nuts securing the air distribution duct to the I/P tie bar. Refer to Air Distributor Duct Replacement.
4. Remove the bolts securing the I/P tie bar to the brake pedal bracket.

1 | I/P Tie Bar Bolts (Qty: 4) Caution: Refer to Fastener Caution in the Preface section. Tighten 25 N·m (18 lb ft)
2 | I/P Tie Bar Bolts (Qty: 2) Tighten 12 N·m (106 lb in)
3 | I/P Tie Bar Assembly