For 1990-2009 cars

## Tail Lamp Replacement Sky

Callout | Component Name
--- | ---

#### Preliminary Procedure

Open the rear compartment lid in order to access the tail lamp screws.

1 | Tail Lamp Assembly Screw (Qty: 2) Caution: Refer to Fastener Caution in the Preface section. Tighten 2.5 N·m (22 lb in)
2 | Chassis Electrical Connector Tip Lift the tail lamp in order to disengage the retainer clips then disconnect the electrical connector.
3 | Tail Lamp Assembly Tip Transfer the bulb into the new tail lamp.
4 | Quarter Filler Panel Nut (Qty: 2) Tip Ensure the quarter filler panel nuts are not damaged. Replace if damaged.

## Tail Lamp Replacement Solstice

Callout | Component Name
--- | ---

#### Preliminary Procedure

Open the rear compartment lid in order to access the tail lamp screws.

1 | Tail Lamp Assembly Screw (Qty: 2) Caution: Refer to Fastener Caution in the Preface section. Tighten 2.5 N·m (40 lb in)
2 | Locating Pin (Qty: 2) Tip Lift upward on the tail lamp assembly in order to release the tail lamp locating pins from the quarter filler panel.
3 | Chassis Electrical Connector Tip Disconnect the electrical connector.
4 | Quarter Filler Panel Nut (Qty: 2) Tip Ensure the quarter filler panel nuts are not damaged. Replace if damaged.
5 | Tail Lamp Assembly Tip Transfer the bulb into the new tail lamp.
6 | Retainer Clip (Qty: 2) Tip Ensure clips are secure to the quarter filler panel.