For 1990-2009 cars

Callout | Component Name
--- | ---

#### Preliminary Procedure

1. Remove the fuse labeled HVAC CTRL (BATT).
2. Remove the knee bolster. Refer to Knee Bolster Replacement.
3. Disconnect the electrical connector.

1 | Screw, Air Temperature Actuator Caution: Refer to Fastener Caution in the Preface section. Tighten 1.5 N·m (13 lb in)
2 | Actuator, Air Temperature - Right

#### Procedure

• | Disconnect the actuator electrical connector.

• | Recalibrate the Actuator. Refer to Actuator Recalibration