For 1990-2009 cars

Callout | Component Name
--- | ---
Notice: Refer to Fastener Notice in the Preface section. Fastener Tightening Specifications: Refer to Fastener Tightening Specifications .

#### Preliminary Procedures

1. Open the folding top and stowage compartment lid.
2. Remove the upper garnish molding. Refer to Windshield Upper Garnish Molding Replacement .

1 | Bolts, Receiver Pin Front Locating Folding Top (Qty: 2) Tip Mark the location of the receiver before removing. Tighten 25 N·m (18 lb ft)
2 | Receiver, Pin Front Locating Folding Top