For 1990-2009 cars

### Removal Procedure

1. Remove the control lever knob and boot assembly. Refer to Control Lever and/or Boot Replacement.
2. Remove the turbocharger, if equipped. Refer to Turbocharger Replacement.
3. Remove the clutch hose/pipe assembly retainer clip (1) from the clutch master cylinder.
4. Disconnect the clutch hose/pipe assembly (2) from the clutch master cylinder.
5. Cap the clutch hose/pipe assembly (2) in order to prevent fluid loss and contamination.

It is not necessary to plug the lower hose end or slave cylinder fitting as they are equipped with check valves, only minimal fluid loss may be experienced.

6. Remove the starter. Refer to Starter Replacement.
7. Remove the transmission support. Refer to Transmission Support Replacement.
8. Drain the transmission fluid if necessary. Refer to Transmission Fluid Replacement.
9. Disconnect the electrical connector (2) from the backup lamp switch (5).
10. Disconnect the electrical connector (3) from the vehicle speed sensor (VSS) (4)
11. Disconnect the wiring harness (1) from the clip bracket.
12. Disconnect the wiring harness clips (6) from the clip brackets, and position the harness aside.
13. Support the transmission using a transmission jack.
14. Remove the propeller shaft and driveline support. Refer to Propeller Shaft, Differential, and Driveline Support Replacement.
15. Remove the 5 transmission to engine mounting bolts (1).
16. Remove the 2 engine to transmission mounting bolts (2).
17. Remove the 2 remaining transmission mounting bolts (2).

Important: Do not allow the transmission to hang from the clutch assembly.

18. Pull the transmission straight back off the clutch hub splines.

Important: Ensure clearance is maintained between the transmission and the following:

• | The catalytic converter

• | The clutch assembly

• | The engine wiring harness

• | The clutch actuator pipe and hose

19. Using the transmission jack, carefully lower the transmission from the vehicle.

### Installation Procedure

Important: Ensure clearance is maintained between the transmission and the following:

• | The catalytic converter

• | The clutch assembly

• | The engine wiring harness

1. Using the transmission jack, carefully raise the transmission to the engine.

Important: Do not allow the transmission to hang from the clutch assembly.

2. Align the transmission with the engine dowels (1).

Notice: Refer to Fastener Notice in the Preface section.

3. Install the 2 transmission mounting bolts (2).

Tighten
Tighten the bolts to 50 N·m (37 lb ft).

4. Install the 2 engine to transmission mounting bolts (2).

Tighten
Tighten the bolts to 50 N·m (37 lb ft).

5. Install the 5 transmission to engine mounting bolts (1).

Tighten
Tighten the bolts to 50 N·m (37 lb ft).

6. Install the driveline support and propeller shaft. Refer to Propeller Shaft, Differential, and Driveline Support Replacement.
7. Remove the transmission jack.
8. Lay the engine wiring harness over the transmission.
9. Connect the wiring harness clips (6) to the clip brackets.
10. Connect the wiring harness (1) to the clip bracket.
11. Connect the electrical connector (3) to the VSS (4)
12. Connect the electrical connector (2) to the backup lamp switch (5).
13. Fill the transmission fluid if removed. Refer to Transmission Fluid Replacement.
14. Install the transmission support and closeout panels. Refer to Transmission Support Replacement.

Important: Ensure the clutch hydraulic hose does not come in contact with any sharp or potentially hot surfaces.

15. Install the clutch hose/pipe assembly retainer clip (2) to the clutch master cylinder.
16. Connect the clutch hose/pipe assembly (3) to the clutch master cylinder.
17. Tug gently on the clutch hose/pipe assembly (3) to ensure proper retention into the clutch master cylinder.
18. Install the turbocharger, if equipped. Refer to Turbocharger Replacement.
19. Install the control lever knob and boot assembly. Refer to Control Lever and/or Boot Replacement.
20. Install the starter. Refer to Starter Replacement.

### Transmission Final Test and Inspection

Complete the following procedure after the transmission is installed in the vehicle:

1. With the ignition OFF or disconnected and clutch pedal depressed, crank the engine several times. Listen for any unusual noises or evidence that any parts are binding.
2. Place the transmission in neutral, start the engine and listen for any unusual noises or evidence that any parts are binding.
3. Turn OFF the ignition.
4. Perform a final inspection for the proper fluid level. Refer to Transmission Fluid Replacement.
5. Road test the vehicle.