For 1990-2009 cars

Callout | Component Name
--- | ---

#### Preliminary Procedures

1. Remove the instrument panel (I/P) accessory trim plate. Refer to Instrument Panel Accessory Trim Plate Replacement.
2. Remove the I/P compartment frame. Refer to Instrument Panel Compartment Door Opening Frame Replacement.
3. Remove the knee bolster assembly. Refer to Knee Bolster Replacement.

1 | I/P Lower Trim Panel Screw Caution: Refer to Fastener Caution in the Preface section. Tighten 2.5 N·m (22 lb in)
2 | I/P Lower Trim Panel Assembly

#### Procedures

1. Disconnect the electrical connectors.
2. When replacing the instrument lower trim panel, transfer all necessary components.

3 | Retainer Clips (Qty: 6)