For 1990-2009 cars

# Chime volume adjustment - keywords int intermittent level loud normal preset radio soft three

Subject: | Chime Volume Adjustment

Models: | 2006-2008 Chevrolet Cobalt

| 2006-2008 Chevrolet HHR

| 2008 Chevrolet Malibu (New body style)

| 2006-2008 Pontiac Solstice

| 2007-2008 Saturn Aura

| 2007-2008 Saturn Sky

The following diagnosis might be helpful if the vehicle exhibits the symptom(s) described in this PI.

### Condition/Concern:

A customer might comment that the audible chimes (headlight,door,key) are too loud and they wish to have the chime volume lowered. Currently there is no procedure in SI to adjust the volume of the Chime.

### Recommendation/Instructions:

Chime Level Adjustment:

The radio is used to adjust the vehicle's chime level. To change the volume level of the chime, press and hold push-button 6 with the ignition on and the radio power off. The volume level will change from the normal level to loud, and LOUD will appear on the radio display. To change back to the default or normal setting, press and hold push-button 6 again. The volume level will change from the loud level to normal, and NORMAL will appear on the radio display.

Note: Each time the chime volume is changed, three chimes will sound to indicate the new volume selected.

Please follow this diagnostic or repair process thoroughly and complete each step. If the condition exhibited is resolved without completing every step, the remaining steps do not need to be performed.