For 1990-2009 cars

Callout | Component Name
--- | ---

#### Preliminary Procedures

1. Raise and support the vehicle. Refer to Lifting and Jacking the Vehicle.
2. Reposition either the left front or right front wheelhouse liner for access to the running lamp. Refer to Front Wheelhouse Liner Replacement.
3. Disconnect the fog lamp bulb socket electrical connector.
4. Disconnect the electrical connector harness for the DRL, Park and Turn Signal socket.

1 | Daytime Running, Park and Turn Signal Lamp Assembly Screw (Qty: 4) Caution: Refer to Fastener Caution in the Preface section. Tighten 2 N·m (18 lb in)
2 | Daytime Running, Park and Turn Signal Lamp Assembly

#### Procedure

1. Transfer the fog lamp assembly to the new DRL lamp assembly. Refer to Front Fog Lamp Replacement.
2. Aim the fog lamp after installation. Refer to Fog Lamp Aiming.