For 1990-2009 cars

## Radiator Support Bracket Replacement LNF

Callout | Component Name
--- | ---
Notice: Refer to Fastener Notice in the Preface section. Fastener Tightening Specifications: Refer to Fastener Tightening Specifications .

#### Preliminary Procedure

Remove the air cleaner assembly. Refer to Air Cleaner Assembly Replacement .

1 | Charge Air Cooler Pipe Bolt Tighten 22 N·m (16 lb ft)
2 | Radiator Upper Bracket Nut (Qty: 2) Tighten 9 N·m (80 lb in)
3 | Charge Air Cooler Pipe Rear Bracket
4 | Air Cleaner Stud Tighten 10 N·m (89 lb in)
5 | Radiator Upper Bracket Assembly

## Radiator Support Bracket Replacement LE5

Callout | Component Name
--- | ---
Notice: Refer to Fastener Notice in the Preface section. Fastener Tightening Specifications: Refer to Fastener Tightening Specifications

#### Preliminary Procedure

Remove the air cleaner assembly. Refer to Air Cleaner Assembly Replacement .

1 | Air Cleaner Stud Tighten 10 N·m (89 lb in)
2 | Radiator Upper Bracket Nut Tighten 9 N·m (80 lb in)
3 | Radiator Upper Bracket Assembly