For 1990-2009 cars

Callout | Component Name
--- | ---

#### Preliminary Procedure

Remove the HVAC module assembly. Refer to HVAC Module Assembly Replacement .

1 | Evaporator Case Seal
2 | Thermal Expansion Valve Bolts (Qty: 2) Notice: Refer to Fastener Notice in the Preface section. Tighten 1.5 N·m (13 lb in)
3 | Thermal Expansion Valve
4 | Sealing Washer Tip Remove and discard seals. Refer to Sealing Washer Replacement .
5 | Rear Air Outlet Duct Screw (Qty: 2) Tighten 1.5 N·m (13 lb in)
6 | Rear Air Outlet Duct
7 | Lower Evaporator Case Assembly Screw (Qty: 9) Tighten 1.5 N·m (13 lb in)
8 | Evaporator Case - Lower
9 | Air Conditioning Evaporator