For 1990-2009 cars

## Instrument Panel Lower Trim Panel Replacement SKY

Callout | Component Name
--- | ---

#### Preliminary Procedures

1. Remove the instrument panel (I/P) accessory trim plate. Refer to Instrument Panel Accessory Trim Plate Replacement .
2. Remove the I/P compartment frame. Refer to Instrument Panel Compartment Door Opening Frame Replacement .
3. Remove the knee bolster assembly. Refer to Knee Bolster Replacement .

1 | I/P Lower Trim Panel Screw Notice: Refer to Fastener Notice in the Preface section. Tighten 2.5 N·m (22 lb in)
2 | I/P Lower Trim Panel Assembly

#### Procedures

1. Disconnect the electrical connectors.
2. When replacing the instrument lower trim panel, transfer all necessary components.

3 | Retainer Clips (Qty: 6)