For 1990-2009 cars

Callout | Component Name
--- | ---
Fastener Tightening Specifications: Refer to Fastener Tightening Specifications.

#### Preliminary Procedure

Remove the rear tail lamp. Refer to Tail Lamp Replacement.

1 | Stop, Tail and Turn Signal Bulb Socket Harness
2 | Stop, Tail and Turn Signal Bulb Tip Pull the bulb straight from the socket in order to remove.
3 | Stop, Tail and Turn Signal Bulb Socket Harness
4 | Stop, Tail and Turn Signal Bulb Tip Pull the bulb straight from the socket in order to remove.
5 | Rear Side Marker Lamp Bulb Harness
6 | Rear Side Marker Lamp Bulb Tip Pull the bulb straight from the socket in order to remove.