For 1990-2009 cars

## Front Side Door Window Regulator Replacement Manual

Callout | Component Name
--- | ---
Notice: Refer to Fastener Notice in the Preface section. Fastener Tightening Specifications: Refer to Fastener Tightening Specifications .

#### Preliminary Procedures

1. Remove the interior trim panel. Refer to Door Trim Panel Replacement .
2. Remove the water deflector. Refer to Door Water Deflector Replacement .
3. Remove the front side door window. Refer to Front Side Door Window Replacement .

1 | Plug, Window Regulator Nut Access Tip Use a plastic flat-bladed tool to remove the plug from the bottom of the door.
2 | Nut, Front Side Door Window Regulator (Qty: 4) Tighten 10 N·m (89 lb in)
3 | Bolt, Front Door Window Regulator (Qty: 3) Tighten 10 N·m (89 lb in)
4 | Regulator, Front Door Manual Window

## Front Side Door Window Regulator Replacement Power

Callout | Component Name
--- | ---
Notice: Refer to Fastener Notice in the Preface section. Fastener Tightening Specifications: Refer to Fastener Tightening Specifications .

#### Preliminary Procedures

1. Remove the interior trim panel. Refer to Door Trim Panel Replacement .
2. Remove the water deflector. Refer to Door Water Deflector Replacement .
3. Remove the front side door window. Refer to Front Side Door Window Replacement .

1 | Plug, Window Regulator Nut Access Tip Use a plastic flat-bladed tool to remove the plug from the bottom of the door.
2 | Nut, Front Side Door Window Regulator (Qty: 4) Tighten 10 N·m (89 lb in)
3 | Bolt, Front Door Window Regulator (Qty: 3) Tighten 10 N·m (89 lb in)
4 | Regulator, Front Door Power Window Tip Disconnect the electrical connector from the regulator.