For 1990-2009 cars

Callout | Component Name
--- | ---
Notice: Refer to Fastener Notice in the Preface section. Fastener Tightening Specifications: Refer to Fastener Tightening Specifications .

#### Preliminary Procedures

1. Open the hood.
2. Release the connector positive assurance (CPA) connector at the headlamp connector.
3. Disconnect the electrical harness from the headlamp assembly prior to removal.

1 | Headlamp Screws (Qty: 4) Tip Hold the lamp assembly to the hood when removing the screws. Tighten 9 N·m (80 lb in)
2 | Headlamp Assembly Tip Adjust the headlamps after servicing the headlamp assembly. Refer to Headlamp Aiming .