For 1990-2009 cars

Callout | Component Name
--- | ---

#### Preliminary Procedures

1. Disconnect the negative battery cable. Refer to Battery Negative Cable Disconnection and Connection.
2. Remove the intake manifold. Refer to Intake Manifold Replacement or Intake Manifold Replacement.

1 | Starter Solenoid Terminal Nut Caution: Refer to Fastener Caution in the Preface section. Tighten 10 N·m (89 lb in)
2 | Positive Battery Cable Terminal
3 | Starter Solenoid "S" Terminal Nut Tighten 3 N·m (27 lb in)
4 | Engine Harness Terminal
5 | Engine Harness Terminal
6 | Starter Motor Bolt (Qty: 2) Tighten 40 N·m (30 lb ft)
7 | Starter Motor