For 1990-2009 cars

Callout | Component Name
--- | ---
Caution: Refer to Fastener Caution in the Preface section. Fastener Tightening Specifications: Refer to Fastener Tightening Specifications.

#### Preliminary Procedure

Remove the front air deflector. Refer to Front Bumper Fascia Air Deflector Replacement.

1 | Bolt, Horn Tighten 10 N·m (89 lb in)
2 | Horn Tip Disconnect the electrical connector.