For 1990-2009 cars

Callout | Component Name
--- | ---
Notice: Refer to Fastener Notice in the Preface section. Fastener Tightening Specifications: Refer to Fastener Tightening Specifications .

#### Preliminary Procedure

Important: Drain only the fluid from the radiator surge tank.

Drain the cooling system. Refer to Cooling System Draining and Filling .

1 | Radiator Surge Tank Cap Assembly
2 | Radiator Surge Tank Retainer
3 | Radiator Surge Tank Nut Tighten 9 N·m (80 lb in)
4 | Radiator Surge Tank Assembly Tip Using J 38185 position radiator surge tank hose clamps aside and remove hoses from the radiator surge tank.