For 1990-2009 cars

## Front Fender Air Extractor Replacement SKY

Callout | Component Name
--- | ---
Notice: The air extractor cannot be removed from the fender without damage to the fender.

#### Preliminary Procedures

1. Remove the fender. Refer to Front Fender Replacement .
2. Paint the fender and the air extractor before assembly. Refer to Basecoat/Clearcoat Paint Systems .
3. The part and surface should be 21°C (70°F) prior to installation. The vehicle part should remain 21°C (70°F) for one hour after assembly to allow adhesive to develop sufficient bond strength.

1 | Fender Panel

#### Procedure

1. Roughen the shaded surface on the back of the fender panel with ScotchBrite™ or 150 grit sand paper. Wipe clean and dry.
2. Apply 3M-4298 adhesion promoter over the roughened surface to fully cover the shaded area on the back of the fender panel. Allow to dry.

2 | Air Extractor

#### Procedure

1. Roughen the shaded surfaces on the front of the air extractor. Wipe clean and dry. Apply 3M-4298 adhesion promoter over the roughened surface of pockets. Allow to dry.
2. Install large and small tape pieces in pockets of the air extractor. Press firmly in place.
3. Place the air extractor over the locating pins on the back of the fender panel.
4. Press the air extractor firmly in place by hand. Use roller to firmly press over tape pocket areas.