For 1990-2009 cars

## Air Conditioning Compressor Replacement LNF

Callout | Component Name
--- | ---

#### Preliminary Procedures

1. Recover the refrigerant. Refer to Refrigerant Recovery and Recharging .
2. Remove the charge air cooler outlet pipe. Refer to Charge Air Cooler Outlet Pipe Replacement .
3. Remove the air cleaner outlet duct. Refer to Air Cleaner Outlet Duct Replacement .
4. Remove the generator. Refer to Generator Replacement .
5. Remove the drive belt. Refer to Drive Belt Replacement .

1 | A/C Compressor and Condenser Hose Assembly Bolt Notice: Refer to Fastener Notice in the Preface section. Tighten 22 N·m (16 lb ft)
2 | Sealing Washer Tip Remove and discard the sealing washer. Refer to Sealing Washer Replacement .
3 | A/C Compressor Bolt (Qty: 3) Tip Tighten the bolts in sequence. Tighten 22 N·m (16 lb ft)
4 | A/C Compressor Assembly

## Air Conditioning Compressor Replacement LE5

Callout | Component Name
--- | ---

#### Preliminary Procedures

1. Recover the refrigerant. Refer to Refrigerant Recovery and Recharging .
2. Remove the air cleaner outlet duct. Refer to Air Cleaner Outlet Resonator Replacement .
3. Remove the generator. Refer to Generator Replacement .
4. Remove the drive belt. Refer to Drive Belt Replacement .

1 | A/C Compressor and Condenser Hose Assembly Bolt Notice: Refer to Fastener Notice in the Preface section. Tighten 22 N·m (16 lb ft)
2 | Sealing Washer Tip Remove and discard the sealing washer. Refer to Sealing Washer Replacement .
3 | A/C Compressor Bolt (Qty: 3) Tip Tighten the bolts in sequence. Tighten 22 N·m (16 lb ft)
4 | A/C Compressor Assembly