For 1990-2009 cars

The floor console fuse block is located on the passenger side of the vehicle under the carpet.

Remove the fuse block cover to access the fuses. Use the fuse puller to remove fuses.

After re-installing the fuse block cover, be sure to tuck the carpet under the heater floor outlets.

Fuses | Usage
--- | ---
1 | Fuse Puller
2 | Empty
3 | Empty
4 | Empty
5 | Empty
6 | Amplifier
7 | Cluster
8 | Ignition Switch, PassKey III+
9 | Stoplamp
10 | Climate Control System, PassKey III+
11 | Empty
12 | Spare
13 | Airbag
14 | Spare
15 | Wiper
16 | Climate Control System, Automatic Occupant Sensing Module, Crank Relay, Instrument Panel Cluster
17 | Empty
18 | Empty
19 | Steering Wheel Controls
20 | Spare
21 | Spare
22 | Empty
23 | Radio
24 | Sensing and Diagnostic Module
25 | Engine Control Module, Transmission Control Module
26 | Door Locks
27 | Interior Lamps
28 | Steering Wheel Control Backlighting
29 | Power Windows
30 | Climate Control System
31 | Empty
32 | Retained Accessory Power