For 1990-2009 cars

Callout | Component Name
--- | ---
Fastener Tightening Specifications: Refer to Fastener Tightening Specifications .

#### Preliminary Procedure

Lift upward, "service up" the wiper arm from the windshield.

1 | Tab, Release Tip From the drivers side of the vehicle, apply downward pressure to the tab and pull wiper blade from the wiper arm hook.
2 | Blade Assembly, Windshield Washer Tip There is a right and left windshield washer blade assembly.