For 1990-2009 cars

## Backup and Rear Fog Lamp Replacement Pontiac

Callout | Component Name
--- | ---
Notice: Refer to Fastener Notice in the Preface section. Fastener Tightening Specifications: Refer to Fastener Tightening Specifications .

#### Preliminary Procedure

Remove either the RR or LR wheelhouse liner. Refer to Rear Wheelhouse Panel Liner Replacement .

1 | Main Body Harness Electrical Connector Tip Squeeze and turn the socket counterclockwise to remove.
2 | Backup and Rear Fog Lamp Assembly Nuts (Qty: 2) Tighten 2.5 N·m (22 lb in)
3 | Backup and Rear Fog Lamp Assembly Tip Remove lamp from exterior side of the rear bumper fascia.