For 1990-2009 cars

## Parking and Turn Signal Lamp Replacement SKY

Callout | Component Name
--- | ---

#### Preliminary Procedure

Remove either the left front or right front wheelhouse liner. Refer to Front Wheelhouse Liner Replacement .

1 | Front Park and Turn Signal and Fog Lamp Assembly Screw (Qty: 4) Notice: Refer to Fastener Notice in the Preface section. Tighten 2 N·m (18 lb in)
2 | Front Park and Turn Signal and Fog Lamp Assembly Tip Disconnect and remove the electrical harness, bulbs and remove the lamp assembly from inside the front bumper fascia.

## Parking and Turn Signal Lamp Replacement Solstice

Callout | Component Name
--- | ---

#### Preliminary Procedures

1. Open the hood.
2. Reach in between the bumper and front hood opening to disconnect the lamp socket electrical connectors.

1 | Park and Turn Signal Lamp Bulb Tip Rotate the bulb socket counterclockwise from the lamp housing in order to remove.
2 | Front Fog Lamp Bulb Tip Rotate the bulb socket counterclockwise from the lamp housing in order to remove.
3 | Front Park and Turn Signal and Fog Lamp Assembly Screw Notice: Refer to Fastener Notice in the Preface section. Tighten 2 N·m (18 lb in)
4 | Front Park and Turn Signal and Fog Lamp Assembly Tip Pull the lamp housing forward in order to remove.