For 1990-2009 cars

Callout | Component Name
--- | ---
Notice: Refer to Fastener Notice in the Preface section. Fastener Tightening Specifications: Refer to Fastener Tightening Specifications .

#### Preliminary Procedures

1. Remove the interior trim panel. Refer to Door Trim Panel Replacement .
2. Remove the water deflector. Refer to Door Water Deflector Replacement .
3. Remove the front side door window. Refer to Front Side Door Window Replacement.
4. Remove the power window regulator. Refer to Front Side Door Window Regulator Replacement.

1 | Bolt, Power Window Motor (Qty: 3) Tighten 10 N·m (89 lb in)
2 | Motor, Power Window Regulator