For 1990-2009 cars

### Removal Procedure

1. Remove the throttle body. Refer to Throttle Body Assembly Replacement .
2. Disconnect the manifold absolute pressure (MAP) sensor electrical connector.
3. Remove the MAP sensor and the MAP sensor port seal if it is still retained in the intake manifold

### Installation Procedure

1. Install the MAP sensor with the port seal into the intake manifold
2. Connect the MAP sensor electrical connector.
3. Install the throttle body. Refer to Throttle Body Assembly Replacement .