For 1990-2009 cars

Callout | Component Name
--- | ---
Notice: Refer to Fastener Notice in the Preface section. Fastener Tightening Specifications: Refer to Fastener Tightening Specifications .

#### Preliminary Procedures

1. Remove the interior trim panel. Refer to Door Trim Panel Replacement .
2. Remove the water deflector. Refer to Door Water Deflector Replacement .

1 | Screw, Front Side Door Lock (Qty: 3) Tip Disconnect the lock cylinder and outside handle rod from the lock assembly. Tighten 10 N·m (89 lb in)
2 | Lock Assembly, Front Side Door Tip

1. Release the door lock cable retainers from the door.
2. Disconnect the door lock electrical connector.