For 1990-2009 cars

# Rattle/Noise in Trunk Area with Convertible Top Stowed (Center Guide Pins or Add Felt Tape)

Subject: | Rattle/Noise in Trunk Area with Convertible Top Stowed (Center Guide Pins or Add Felt Tape)

Models: | 2006-2008 Pontiac Solstice

| 2007-2008 Saturn Sky

| 2007-2008 Opel GT

| 2008 Daewoo G2X

This bulletin is being updated to add models and model years. Please discard Corporate Bulletin Number 06-08-67-018 (Section 08 - Body and Accessories).

### Condition

Some customers may comment that there is a rattle in the trunk area with the top stowed.

### Cause

This condition may be caused by the convertible top guide pins not being centered in their pockets or the felt may be missing from the pocket.

### Correction

Lower the top to the almost seated position. Slightly bend the pocket with pliers until it is centered with the pin or add BSR felt tape (KT13296 from Kent).

### Warranty Information

For vehicles repaired under warranty, use:

Labor Operation | Description | Labor Time
--- | --- | ---
C9773* | Adjust Pin and Pocket | 0.2 hr
*This is a unique labor operation for bulletin use only. It will not be published in the Labor Time Guide.