For 1990-2009 cars

## Fascia Grille Replacement Solstice

Callout | Component Name
--- | ---
Fastener Tightening Specifications: Refer to Fastener Tightening Specifications.

#### Preliminary Procedure

Remove the front fascia. Refer to Front Bumper Fascia Replacement

1 | Retainer Clips, Front Fascia Grille (Qty: 4)
2 | Grille, Front Fascia Tip Using a flat bladed tool, pry the grille out of the fascia.

## Fascia Grille Replacement Solstice Turbo Center Grille

Callout | Component Name
--- | ---

#### Preliminary Procedure

Remove the front fascia. Refer to Front Bumper Fascia Replacement

1 | Front Fascia Grille Retainer Clips (Qty: 3)
2 | Front Fascia Grille Tip Using a flat bladed tool, pry the grille out of the fascia.

## Fascia Grille Replacement Solstice Turbo Lower Grille

Callout | Component Name
--- | ---
1 | Front Fascia Grille Plastic Rivets (Qty: 6)
2 | Front Fascia Lower Grille Tip Remove the plastic rivets and push the upper edge of the grille rearward off the mounting tabs and pull the grille forward in order to remove.

## Fascia Grille Replacement Solstice Turbo Outer Grille

Callout | Component Name
--- | ---
1 | Front Fascia Outer Grille Screw (Qty: 2) Notice: Refer to Fastener Notice in the Preface section. Tighten 2 N·m (18 lb in)
2 | Front Fascia Outer Grille Tip Move the inside of the grille outward in order to release the inner locking tab from the front bumper fascia.