For 1990-2009 cars

Callout | Component Name
--- | ---

#### Preliminary Procedures

1. Remove the air cleaner assembly. Refer to Air Cleaner Assembly Replacement.
2. Remove the side radiator air lower baffle and deflector. Refer to Radiator Air Lower Baffle and Deflector Replacement.
3. Remove the radiator upper air baffle and deflector. Refer to Radiator Air Upper Baffle and Deflector Replacement.

1 | Power Steering Gear Outlet Hose Clamp

#### Procedure

Remove as much power steering fluid as possible from the remote power steering fluid reservoir.

2 | Power Steering Gear Outlet Hose
3 | Power Steering Fluid Cooler Hose Clamp
4 | Power Steering Fluid Cooler Hose
5 | Power Steering Fluid Cooler Pipe Bracket Bolt (Qty: 2) Caution: Refer to Fastener Caution in the Preface section. Tighten 9 N·m (80 lb in)
6 | Power Steering Fluid Cooler

#### Procedure

1. Remove the power steering fluid cooler from the bottom of the vehicle.
2. Fill and bleed the power steering system. Refer to Power Steering System Bleeding