For 1990-2009 cars

Callout | Component Name
--- | ---

#### Preliminary Procedure

1. Remove the rear compartment trim. Refer to Rear Compartment Trim Panel Replacement .
2. Remove the right rear wheelhouse panel. Refer to Rear Wheelhouse Panel Liner Replacement .

1 | Antenna Assembly, Radio
2 | Nut, Radio Antenna Base Notice: Refer to Fastener Notice in the Preface section. Tighten 2 N·m (18 lb in)
3 | Cap, Radio Antenna Bracket Stud
4 | Bolt, Radio Antenna Tighten 10 N·m (89 lb in)
5 | Bracket Assembly, Radio Antenna