For 1990-2009 cars

Callout | Component Name
--- | ---
Caution: Refer to Fastener Caution in the Preface section. Fastener Tightening Specifications: Refer to Fastener Tightening Specifications.

#### Preliminary Procedure

1. Remove the fuse labeled HVAC CTRL (BATT).
2. Remove the air inlet assembly. Refer to Air Inlet Assembly Replacement.
3. Disconnect the recirculation actuator electrical connector.

1 | Screw, Recirculation Housing (Qty: 4) Tighten 1.5 N·m (14 lb in)
2 | Housing, Recirculation
3 | Screw, Recirculation Actuator (Qty: 3) Tighten 1.5 N·m (13 lb in)
4 | Actuator, Recirculation

#### Procedure

• | Disconnect the actuator electrical connector.

• | Recalibrate the Actuator. Refer to Actuator Recalibration