For 1990-2009 cars

Callout | Component Name
--- | ---
Notice: Refer to Fastener Notice in the Preface section.

#### Preliminary Procedure

Remove either the LF or Rf wheelhouse liner. Refer to Front Wheelhouse Liner Replacement .

1 | Front Park and Turn Signal and Fog Lamp Assembly Screws (Qty: 4) Tighten 2 N·m (18 lb in)
2 | Front Park and Turn Signal and Fog Lamp Assembly Tip Disconnect and remove the electrical harness, bulbs and remove the lamp assembly from inside the front bumper fascia.