For 1990-2009 cars

## Radiator Surge Tank Outlet Hose/Pipe Replacement LNF

Callout | Component Name
--- | ---

#### Preliminary Procedure

1. Drain the cooling system. Refer to Cooling System Draining and Filling .
2. Remove the air inlet grill panel. Refer to Air Inlet Grille Panel Replacement .

1 | Radiator Surge Tank Hose Assembly - Outlet Tip Using SA9111E position radiator surge tank outlet hose clamps aside and remove hose from the fittings.

## Radiator Surge Tank Outlet Hose/Pipe Replacement LE5

Callout | Component Name
--- | ---
Caution: Refer to Fastener Caution in the Preface section. Fastener Tightening Specifications: Refer to Fastener Tightening Specifications.

#### Preliminary Procedure

1. Drain the cooling system. Refer to Cooling System Draining and Filling.
2. Remove the air inlet grill panel. Refer to Air Inlet Grille Panel Replacement.

1 | Hose Assembly, Radiator Surge Tank Outlet Tip Using J 38185 position radiator surge tank outlet hose clamps aside and remove hose from the fittings.