For 1990-2009 cars

## Knee Bolster Replacement Sky

Callout | Component Name
--- | ---

#### Preliminary Procedures

1. Remove the left instrument panel closeout/insulator panel. Refer to Instrument Panel Insulator Panel Replacement - Left Side.
2. Remove the left instrument panel outer trim cover. Refer to Instrument Panel Outer Trim Cover Replacement.

1 | Knee Bolster Screw (Qty: 4) Caution: Refer to Fastener Caution in the Preface section. Tighten 2.5 N·m (22 lb in)
2 | Knee Bolster Assembly

#### Procedures

1. Disconnect the electrical connectors.
2. When replacing the knee bolster assembly, transfer all necessary components.

3 | Retainer Clips (Qty: 3)

## Knee Bolster Replacement Solstice

Callout | Component Name
--- | ---

#### Preliminary Procedure

Remove the left instrument panel (I/P) insulator. Refer to Instrument Panel Insulator Panel Replacement - Left Side.

1 | I/P Driver Knee Bolster Screw (Qty: 2) Caution: Refer to Fastener Caution in the Preface section. Tighten 2 N·m (18 lb in)
2 | I/P Driver Knee Bolster Panel Assembly