For 1990-2009 cars

## Instrument Cluster Replacement Solstice

Callout | Component Name
--- | ---

#### Preliminary Procedure

Remove the instrument panel (I/P) cluster Bezel. Refer to Instrument Cluster Trim Panel Replacement.

1 | I/P Cluster Screw (Qty: 4) Caution: Refer to Fastener Caution in the Preface section. Tighten 2 N·m (18 lb in)
2 | I/P Cluster Assembly Tip Refer to Control Module References for programming and setup information.

## Instrument Cluster Replacement SKY

Callout | Component Name
--- | ---

#### Preliminary Procedure

Remove the instrument panel (I/P) upper trim panel. Refer to Instrument Panel Upper Trim Panel Replacement.

1 | I/P Cluster Assembly Screw (Qty: 4) Caution: Refer to Fastener Caution in the Preface section. Tighten 2 N·m (18 lb in)
2 | I/P Cluster Assembly

#### Procedure

1. Disconnect the electrical connector.
2. When replacing the cluster, refer to Control Module References.