For 1990-2009 cars

Callout | Component Name
--- | ---
Notice: Refer to Fastener Notice in the Preface section. Fastener Tightening Specifications: Refer to Fastener Tightening Specifications .

#### Preliminary Procedure

1. Remove the air cleaner assembly. Refer to Air Cleaner Assembly Replacement .
2. Remove the air cleaner duct. Refer to Air Cleaner Outlet Resonator Replacement .
3. Disconnect the cooling fan motor electrical connector.

1 | Bolt, Radiator Assembly Tighten 25 N·m (18 lb ft).
2 | Shroud Assembly, Cooling Fan and Motor