For 1990-2009 cars

Notice: Never attempt to remove the intake manifold from a hot engine, allow the engine to cool to ambient temperature. The intake manifold is made of a composite plastic and can be damaged if it is removed when the engine is hot.

1. Remove the evaporative emission (EVAP) canister valve tube (1).
2. Remove the EVAP canister valve (2).
3. Remove the throttle body bolts.
4. Remove the throttle body.
5. Remove fuel pipes and clips.
6. Remove the fuel rail bolts.
7. Remove the fuel rail.
8. Remove the fuel injector tip insulators and discard.
9. Remove the intake manifold retaining nuts and bolts.
10. Remove the intake manifold.
11. Remove the intake manifold gasket, if necessary. The gasket can be used again if it is not damaged.