For 1990-2009 cars

#### Tools Required

J 35268-A Camshaft/Front Main Seal Installer

### Removal Procedure

1. Remove the crankshaft balancer. Refer to Crankshaft Balancer Replacement .
2. Using a flat-bladed tool, remove the oil seal from the front cover.

### Installation Procedure

1. Use the J 35268-A in order to install the oil seal to the front cover.
2. Install the crankshaft balancer. Refer to Crankshaft Balancer Replacement .