For 1990-2009 cars

Callout | Component Name
--- | ---

#### Preliminary Procedures

1. Remove the interior trim panel. Refer to Door Trim Panel Replacement .
2. Remove the water deflector. Refer to Door Water Deflector Replacement .
3. Remove the front side door window. Refer to Front Side Door Window Replacement .

1 | Window Regulator Nut Access Plug Tip Use a plastic flat-bladed tool to remove the plug from the bottom of the door.
2 | Front Side Door Window Regulator Nut (Qty: 4) Notice: Refer to Fastener Notice in the Preface section. Tighten 10 N·m (89 lb in)
3 | Front Door Window Regulator Bolt (Qty: 3) Tighten 10 N·m (89 lb in)
4 | Front Door Power Window Regulator Tip Disconnect the electrical connector from the regulator.