For 1990-2009 cars

Callout | Component Name
--- | ---
1 | Roof Lift Off Panel/Window Rear Weatherstrip Screw (Qty :4) Caution: Refer to Fastener Caution in the Preface section. Tighten 2 N·m (18 lb in)
2 | Roof Lift Off Panel/Window Rear Weatherstrip Retainer (Qty :2)
3 | Roof Lift Off Panel/Window Rear Weatherstrip

#### Procedure

1. Use a plastic flat-bladed tool to assist in the removal of the weatherstrips two-way tape from the body.
2. Clean the surface using a clean lint free cloth with naphtha or a 50/50 mixture of isopropyl alcohol and water to clean and remove the adhesive film.
3. Ensure the fit of the roof lift off panel/rear window weatherstrip to the weatherstrip retainers is correct before installing the two-way tape to the body and the retainers, to avoid water leaks.