For 1990-2009 cars

Callout | Component Name
--- | ---
Fastener Tightening Specifications: Refer to Fastener Tightening Specifications .

#### Preliminary Procedure

Open and support the hood.

1 | Side Marker Lamp Bulb Tip Twist the lamp socket counter-clockwise and pull the bulb straight out from the socket.
2 | Headlamp Bulb (Lo Beam) Tip Disconnect the electrical connector prior to removing the bulb.
3 | Headlamp Bulb (Hi Beam) Tip Disconnect the electrical connector prior to removing the bulb.
4 | Headlamp Bulb Accessory Cover (Qty: 2) Tip Turn the accessory bulb covers a quarter turn counter-clockwise and remove.