For 1990-2009 cars

Callout | Component Name
--- | ---
Caution: Refer to Fastener Caution in the Preface section. Fastener Tightening Specifications: Refer to Fastener Tightening Specifications.

#### Preliminary Procedure

1. Remove the instrument panel (I/P) compartment. Refer to Instrument Panel Compartment Replacement.
2. Disconnect the blower motor resistor electrical connector.

1 | Screw, Blower Motor Resistor (Qty: 2) Tighten 1.5 N·m (13 lb in)
2 | Resistor, Blower Motor
3 | Screw, Blower Motor (Qty: 3) Tighten 1.5 N·m (13 lb in)
4 | Motor Assembly, Blower